{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":2419,"n_cols":8,"rows_kept":2419,"merged":[[0,0,0,7],[2,0,2,7],[3,0,3,7]],"flags":["formulas_cached_only"]}
["泰州体育公园体育馆、游泳馆、健身馆、热源中心、体育场暖通材料清单"]
["序号","材料（设备）名称","规格型号","单位","工程量","单价（含税13%、含运费）","合计总价（元）","备注"]
["体育公园通风设备"]
["地下商业"]
[1,"70°防火阀","500*320","个",3]
[2,"70°防火阀","400*250","个",1]
[3,"70°防火阀","400*200","个",1]
[4,"70°防火阀","250*120","个",1]
[5,"70°防火阀","630*800","个",1]
[6,"70°防火阀","1000*320","个",2]
[7,"70°防火阀","1200*500","个",2]
[8,"70°防火阀","800*400","个",1]
[9,"70°防火阀","1000*400","个",1]
[10,"70°防火阀","1200*500","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[11,"70°防火阀","320*160","个",3,null,null,"常开70°熔断关闭"]
[12,"70°防火阀","250*160","个",2,null,null,"常开70°熔断关闭"]
[13,"70°防火调节阀","500*320","个",1]
[14,"常闭送风阀","1000*500","个",2,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[15,"常闭送风阀","630*400","个",1,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[16,"常闭送风阀","800*320","个",3,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[17,"常闭送风阀","800*400","个",1,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[18,"单层百叶风口","200*200","个",11]
[19,"单层百叶风口","500*250","个",1]
[20,"单层百叶风口","1100*630","个",3]
[21,"单层百叶风口","1000*600","个",2]
[22,"单层百叶风口","250*250","个",1]
[23,"单层百叶风口","300*300","个",1]
[24,"单层百叶风口","500*250","个",1]
[25,"单层百叶风口","200*200","个",1]
[26,"单层百叶风口","600*400","个",3]
[27,"单层百叶风口","500*320","个",1]
[28,"单层百叶风口","1250*500","个",1]
[29,"单层百叶风口","800*1450","个",1]
[30,"单层百叶风口","1250*500","个",2]
[31,"单层百叶风口","500*320","个",5]
[32,"单层百叶风口","400*320","个",1]
[33,"单层百叶风口","800*400","个",2]
[34,"单层百叶风口","250*500","个",1]
[35,"单层百叶风口","250*200","个",2]
[36,"单层百叶风口","500*320","个",2]
[37,"单层百叶风口","250*200","个",12]
[38,"单层百叶风口","800*400","个",8]
[39,"单层百叶风口","200*200","个",11]
[40,"单层百叶风口","1000*1100","个",1]
[41,"单层百叶风口","630*1000","个",1]
[42,"单层百叶风口","320*200","个",6]
[43,"单层百叶风口","800*400","个",10]
[44,"单层百叶风口","800*630","个",3]
[45,"单层百叶风口","800*1100","个",1]
[46,"单层百叶风口","630*400","个",2]
[47,"单层百叶风口带调节阀","800*400","个",2]
[48,"单层百叶风口带调节阀","630*500","个",8]
[49,"单层百叶风口带调节阀","800*400","个",5]
[50,"单层百叶风口带调节阀","800*400","个",6]
[51,"单层百叶风口带调节阀","800*400","个",6]
[52,"单层百叶风口带调节阀","1000*500","个",6]
[53,"单层百叶风口带调节阀","630*400","个",1]
[54,"单层百叶风口带调节阀","1000*500","个",4]
[55,"单层百叶风口带调节阀","800*400","个",5]
[56,"单层百叶风口带调节阀","800*320","个",5]
[57,"单层百叶风口带调节阀","800*320","个",5]
[58,"单层百叶风口带调节阀","800*400","个",2]
[59,"单层百叶风口带调节阀","1000*500","个",4]
[60,"单层百叶风口带调节阀","630*400","个",8]
[61,"单层百叶风口带调节阀","800*500","个",4]
[62,"单层百叶风口带调节阀"," 250*160","个",1]
[63,"单层百叶风口带调节阀","600*400","个",4]
[64,"蛋格型风口","600*600","个",10,null,null,"带调节阀"]
[65,"电动双位阀","630*400","个",1]
[66,"电动双位阀","630*400","个",1]
[67,"电动调节阀","630*400","个",1]
[68,"电动调节阀","1800*500","个",1]
[69,"电动调节阀","1000*1000","个",1]
[70,"电动调节阀","1800*500","个",1]
[71,"电动调节阀","1400*800","个",1]
[72,"电动调节阀","1800*500","个",1]
[73,"电动调节阀","1500*800","个",1]
[74,"电动调节阀","1800*500","个",1]
[75,"电动调节阀","1250*1000","个",1]
[76,"电动调节阀","1800*500","个",1]
[77,"电动调节阀","1400*800","个",1]
[78,"电动调节阀","1800*500","个",1]
[79,"电动调节阀","1250*800","个",1]
[80,"电动调节阀","1250*500","个",1]
[81,"电动调节阀","1000*500","个",1]
[82,"电动调节阀","1250*630","个",1]
[83,"电动调节阀","1250*630","个",1]
[84,"防火阀","1000*1250","个",1,null,null,"常开70°熔断关闭"]
[85,"防火阀","630*800","个",1,null,null,"常开70°熔断关闭"]
[86,"防火阀","1000*1250","个",1,null,null,"常开70°熔断关闭"]
[87,"防火阀","1000*1250","个",1,null,null,"常开70°熔断关闭"]
[88,"防火阀","630*800","个",1,null,null,"常开70°熔断关闭"]
[89,"防火阀","1000*1250","个",1,null,null,"常开70°熔断关闭"]
[90,"防火阀","1000*800","个",1,null,null,"常开70°熔断关闭"]
[91,"防火阀","1000*800","个",1,null,null,"常开70°熔断关闭"]
[92,"防火阀","1250*500","个",2,null,null,"常开70°熔断关闭"]
[93,"防火阀","800*400","个",1,null,null,"常开70°熔断关闭"]
[94,"防火阀","400*160","个",3,null,null,"常开70°熔断关闭"]
[95,"防火阀","630*500","个",1,null,null,"常开70°熔断关闭"]
[96,"防火阀","800*400","个",2,null,null,"常开70°熔断关闭"]
[97,"防火阀","1000*1250","个",1,null,null,"常开70°熔断关闭"]
[98,"防火阀","500*630","个",1,null,null,"常开70°熔断关闭"]
[99,"防火阀","400*630","个",1,null,null,"常开70°熔断关闭"]
[100,"防火阀","800*320","个",2,null,null,"常开70°熔断关闭"]
[101,"防火阀","630*400","个",2,null,null,"常开70°熔断关闭"]
[102,"防火阀","1800*500","个",1,null,null,"常开70°熔断关闭"]
[103,"防火阀","1800*630","个",1,null,null,"常开70°熔断关闭"]
[104,"防火阀","2000*630","个",1,null,null,"常开70°熔断关闭"]
[105,"防火阀","1800*500","个",1,null,null,"常开70°熔断关闭"]
[106,"防火阀","1400*800","个",1,null,null,"常开70°熔断关闭"]
[107,"防火阀","2000*630","个",1,null,null,"常开70°熔断关闭"]
[108,"防火阀","1800*500","个",1,null,null,"常开70°熔断关闭"]
[109,"防火阀","1500*800","个",1,null,null,"常开70°熔断关闭"]
[110,"防火阀","2000*630","个",1,null,null,"常开70°熔断关闭"]
[111,"防火阀","1800*500","个",1,null,null,"常开70°熔断关闭"]
[112,"防火阀","1250*1000","个",1,null,null,"常开70°熔断关闭"]
[113,"防火阀","2000*630","个",1,null,null,"常开70°熔断关闭"]
[114,"防火阀","1800*500","个",1,null,null,"常开70°熔断关闭"]
[115,"防火阀","1400*800","个",1,null,null,"常开70°熔断关闭"]
[116,"防火阀","2000*630","个",1,null,null,"常开70°熔断关闭"]
[117,"防火阀","1800*500","个",1,null,null,"常开70°熔断关闭"]
[118,"防火阀","1250*800","个",1,null,null,"常开70°熔断关闭"]
[119,"防火阀","2000*630","个",1,null,null,"常开70°熔断关闭"]
[120,"防火阀","800*320","个",2,null,null,"常开70°熔断关闭"]
[121,"防火阀","630*400","个",1,null,null,"常开70°熔断关闭"]
[122,"防火阀","1000*500","个",2,null,null,"常开70°熔断关闭 带返回信号"]
[123,"防火阀","1250*500","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[124,"防火阀","630*500","个",1,null,null,"常开70°熔断关闭"]
[125,"防火阀","630*400","个",1,null,null,"常开70°熔断关闭"]
[126,"防火阀","1250*630","个",1,null,null,"常开70°熔断关闭"]
[127,"防火阀","1800*630","个",1,null,null,"常开70°熔断关闭"]
[128,"防火阀","1600*630","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[129,"防火阀","800*320","个",4]
[130,"防火阀","630*400","个",2,null,null,"常开70°熔断关闭"]
[131,"防火风口","500*600","个",1,null,null,"70°熔断关闭"]
[132,"防火风口","400*800","个",1,null,null,"70°熔断关闭"]
[133,"防火风口","400*250","个",2,null,null,"70°熔断关闭"]
[134,"防火风口","200*200","个",1,null,null,"70°熔断关闭"]
[135,"防火风口","630*400","个",2,null,null,"70°熔断关闭"]
[136,"防火调节阀","800*400","个",2,null,null,"常开70°熔断关闭 带风量调节功能"]
[137,"防火调节阀","630*500","个",1,null,null,"常开70°熔断关闭 带风量调节功能"]
[138,"防烟防火风口","600*1400","个",1,null,null,"常开70°熔断关闭带风量调节带返回信号"]
[139,"防烟防火风口","250*250","个",2,null,null,"常开70°熔断关闭带风量调节 信号或手动关闭 带返回信号"]
[140,"防烟防火风口","400*800","个",1,null,null,"常开70°熔断关闭带风量调节带返回信号"]
[141,"防烟防火风口","600*1000","个",2,null,null,"常开70°熔断关闭带风量调节带返回信号"]
[142,"防烟防火调节阀","800*400","个",3,null,null,"常开信号输出70°熔断关闭带调节阀"]
[143,"防烟防火调节阀","400*200","个",1]
[144,"防烟防火调节阀","1250*630","个",1,null,null,"常开信号输出70°熔断关闭带调节阀"]
[145,"防烟防火调节阀","1250*630","个",1,null,null,"常开信号输出70°熔断关闭带调节阀"]
[146,"防烟防火调节阀","500*400","个",1,null,null,"常开70°熔断关闭 带返回信号 带调节阀"]
[147,"防烟防火调节阀","630*320","个",1,null,null,"常开70°熔断关闭 带返回信号 带调节阀"]
[148,"防烟防火调节阀","500*250","个",1,null,null,"常开70°熔断关闭 带返回信号 带调节阀"]
[149,"防烟防火调节阀","500*200","个",1,null,null,"常开70°熔断关闭 带返回信号 带调节阀"]
[150,"防烟防火调节阀","1000*500","个",1,null,null,"常开70°熔断关闭带风量调节带返回信号"]
[151,"防烟防火调节阀","800*320","个",6,null,null,"常开70°熔断关闭带风量调节带返回信号"]
[152,"防雨百叶风口","1250*500","个",1]
[153,"防雨百叶风口","2800*630","个",1]
[154,"防雨百叶风口","2800*630","个",1]
[155,"防雨百叶风口","3000*630","个",1]
[156,"防雨百叶风口","3000*630","个",1]
[157,"防雨百叶风口","2800*630","个",1]
[158,"防雨百叶风口","2800*630","个",1]
[159,"防雨百叶风口","1250*500","个",1]
[160,"防雨百叶风口","2000*500","个",1]
[161,"柜式离心防爆风机","5600m3/h 344pa静264pa 900rpm 1.5kw 60db(B)","个",1]
[162,"柜式离心风机","8250m3/h 316pa静225pa 700rpm 3kw 61db(B)","个",1]
[163,"柜式离心风机","18590m3/h 477pa静374pa 650rpm 7.5kw 61db(B)","个",1]
[164,"柜式离心风机","21010m3/h 457pa静376pa 700rpm 7.5kw 69db(B)","个",1]
[165,"柜式离心风机","2880m3/h 256pa静193pa 1000rpm 0.75kw 59db(B)","个",1]
[166,"柜式离心风机","1400m3/h 210pa静190pa 900rpm 0.18kw 58db(B)","个",1]
[167,"柜式离心风机","7500m3/h 320pa静238pa 700rpm 3kw 61db(B)","个",1]
[168,"柜式离心风机","9120m3/h 313pa静255pa 600rpm 3kw 61db(B)","个",1]
[169,"柜式离心风机","21010m3/h 457pa静376pa 700rpm 7.5kw 69db(B)","个",1]
[170,"柜式离心风机","18590m3/h 477pa静374pa 650rpm 7.5kw 61db(B)","个",1]
[171,"柜式离心风机","8660m3/h 429pa静325pa 800rpm 3kw 62db(B)","个",1]
[172,"柜式离心风机","13050m3/h 320pa静240pa 550rpm 4kw 69db(B)","个",1]
[173,"柜式离心风机","18590m3/h 477pa静374pa 650rpm 7.5kw 61db(B)","个",1]
[174,"柜式离心风机","8250m3/h 316pa静225pa 700rpm 3kw 61db(B)","个",1]
[175,"柜式离心风机","16250m3/h 438pa静325pa 650rpm 5.5kw 69db(B)","个",1]
[176,"柜式离心风机","4280m3/h 344pa静205pa 1200rpm 1.1kw 60db(B)","个",1]
[177,"可开铰链式百叶","1250*400","个",9,null,null,"带过滤网"]
[178,"可开铰链式百叶","1000*400","个",1]
[179,"离心式管道风机","860m3/h 330pa静302pa 1380rpm 0.25kw 61db(B)","个",1]
[180,"离心式管道风机","560m3/h 142pa 90w 220V","个",1]
[181,"门铰型蛋格式回风口","1000*800","个",4]
[182,"门铰型蛋格式回风口","1000*800","个",4]
[183,"门铰型蛋格式回风口","1000*800","个",4]
[184,"门铰型蛋格式回风口","1000*800","个",4]
[185,"门铰型蛋格式回风口","1000*800","个",4]
[186,"门铰型蛋格式回风口","1000*1000","个",2]
[187,"门铰型蛋格式回风口","1000*630","个",2]
[188,"门铰型蛋格式回风口","1250*500","个",2]
[189,"排烟阀","630*400","个",1,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[190,"排烟阀","800*400","个",4,null,null,"常闭信号开启及远程手动"]
[191,"排烟阀","800*400","个",5,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[192,"排烟阀","1250*630","个",1,null,null,"常闭信号开启及远程手动"]
[193,"排烟阀","630*500","个",1,null,null,"常闭信号开启及远程手动"]
[194,"排烟阀","800*400","个",1,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[195,"排烟阀","800*400","个",4,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[196,"排烟阀","1250*630","个",1,null,null,"常闭70°熔断关闭信号开启及远程手动"]
[197,"排烟阀","800*400","个",2,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[198,"排烟阀","1000*500","个",1,null,null,"常闭信号开启及远程手动70°熔断关闭"]
[199,"排烟防火阀","630*400","个",1,null,null,"常开280°熔断关闭"]
[200,"排烟防火阀","800*400","个",4,null,null,"常开280°熔断关闭"]
[201,"排烟防火阀","1500*630","个",1,null,null,"常开280°熔断关闭"]
[202,"排烟防火阀","800*400","个",5,null,null,"常开280°熔断关闭"]
[203,"排烟防火阀","320*160","个",2,null,null,"常开280°熔断关闭"]
[204,"排烟防火阀","1250*800","个",1,null,null,"常开280°熔断关闭"]
[205,"排烟防火阀","1500*630","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[206,"排烟防火阀","1500*630","个",1,null,null,"常开280°熔断关闭"]
[207,"排烟防火阀","1250*800","个",1,null,null,"常开280°熔断关闭"]
[208,"排烟防火阀","1500*630","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[209,"排烟防火阀","1500*630","个",1,null,null,"常开280°熔断关闭"]
[210,"排烟防火阀","1250*800","个",1,null,null,"常开280°熔断关闭"]
[211,"排烟防火阀","1500*630","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[212,"排烟防火阀","1250*800","个",1,null,null,"常开280°熔断关闭"]
[213,"排烟防火阀","1500*630","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[214,"排烟防火阀","1500*630","个",1,null,null,"常开280°熔断关闭"]
[215,"排烟防火阀","1250*500","个",1,null,null,"常开280°熔断关闭"]
[216,"排烟防火阀","1250*500","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[217,"排烟防火阀","630*500","个",1,null,null,"常开280°熔断关闭"]
[218,"排烟防火阀","800*400","个",1,null,null,"常开280°熔断关闭"]
[219,"排烟防火阀","800*500","个",2,null,null,"常开280°熔断关闭"]
[220,"排烟防火阀","1250*800","个",1,null,null,"常开280°熔断关闭"]
[221,"排烟防火阀","1500*500","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[222,"排烟防火阀","1000*630","个",1,null,null,"常开280°熔断关闭"]
[223,"排烟防火阀","1100*500","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[224,"排烟防火阀","1100*500","个",1,null,null,"常开280°熔断关闭"]
[225,"排烟防火阀","800*400","个",4,null,null,"常开280°熔断关闭"]
[226,"排烟防火阀","800*400","个",5]
[227,"排烟防火阀","800*400","个",5,null,null,"常开280°熔断关闭 带返回信号"]
[228,"排烟防火阀","1250*630","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[229,"排烟防火阀","1400*630","个",1,null,null,"常开280°熔断关闭"]
[230,"排烟防火阀","630*1000","个",1]
[231,"排烟防火阀","1000*800","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[232,"排烟防火阀","800*400","个",2,null,null,"常开280°熔断关闭"]
[233,"排烟防火阀","1000*500","个",1,null,null,"常开280°熔断关闭"]
[234,"排烟防火风口","800*500","个",2,null,null,"常开信号输出70°熔断关闭带调节阀"]
[235,"排烟防火风口","1000*500","个",2,null,null,"常开信号输出70°熔断关闭带调节阀"]
[236,"排烟防火调节阀","400*200","个",1,null,null,"常开信号输出70°熔断关闭 带风量调节"]
[237,"排烟防火调节阀","400*320","个",1,null,null,"常开信号输出70°熔断关闭 带风量调节"]
[238,"排烟防火调节阀","320*320","个",1,null,null,"常开信号输出70°熔断关闭 带风量调节"]
[239,"双层百叶风口","500*250","个",24]
[240,"双层百叶风口","500*250","个",24]
[241,"双层百叶风口","500*250","个",27]
[242,"双层百叶风口","500*250","个",27]
[243,"双层百叶风口","500*250","个",28]
[244,"双层百叶风口","500*250","个",29]
[245,"双层百叶风口","500*200","个",13]
[246,"双层百叶风口","500*250","个",25]
[247,"条形散流器","1000*171","个",7]
[248,"条形散流器","1000*171","个",1]
[249,"条形散流器","1000*171","个",23]
[250,"调节阀","250*200","个",11]
[251,"调节阀","630*320","个",1]
[252,"调节阀","1000*400","个",1]
[253,"调节阀","1000*400","个",1]
[254,"调节阀","800*400","个",1]
[255,"调节阀","500*250","个",3]
[256,"调节阀","800*500 ","个",1]
[257,"调节阀","500*200","个",1]
[258,"调节阀","400*200","个",3]
[259,"调节阀","1000*400","个",2]
[260,"调节阀","630*320","个",2]
[261,"调节阀","500*200","个",4]
[262,"调节阀","800*320","个",3]
[263,"调节阀","630*400","个",1]
[264,"调节阀","800*320","个",5]
[265,"调节阀","800*400","个",1]
[266,"调节阀","630*200","个",1]
[267,"调节阀","500*200","个",2]
[268,"调节阀","800*320","个",4]
[269,"调节阀","1000*400","个",1]
[270,"调节阀","630*200","个",3]
[271,"调节阀","500*200","个",3]
[272,"调节阀","800*320","个",4]
[273,"调节阀","630*160","个",2]
[274,"调节阀","630*250","个",1]
[275,"调节阀","630*160","个",2]
[276,"调节阀","400*160","个",1]
[277,"调节阀","800*400","个",1]
[278,"调节阀","800*320","个",5]
[279,"调节阀","630*250","个",1]
[280,"调节阀","630*160","个",1]
[281,"调节阀","630*200","个",1]
[282,"调节阀","500*200","个",2]
[283,"调节阀","800*400","个",1]
[284,"调节阀","800*320","个",5]
[285,"调节阀","400*320","个",1]
[286,"调节阀","250*200","个",10]
[287,"调节阀","320*200","个",1]
[288,"调节阀","630*200","个",1]
[289,"调节阀","500*200","个",2]
[290,"调节阀","630*200","个",3]
[291,"调节阀","320*200","个",6]
[292,"调节阀","630*250","个",6]
[293,"调节阀","630*250","个",1]
[294,"调节阀","500*200","个",1]
[295,"调节阀","800*400","个",1]
[296,"调节阀","800*320","个",3]
[297,"调节阀","320*250","个",7]
[298,"调节阀","500*200","个",1]
[299,"消防高温排烟风机","48500m3/h 690pa 1450rpm 15kw 93db(B)","个",1]
[300,"消防高温排烟风机","57748m3/h 740pa 960rpm 18.5kw 93db(B)","个",1]
[301,"消防高温排烟风机","46658m3/h 726pa 1450rpm 15kw 93db(B)","个",1]
[302,"消防高温排烟风机","48500m3/h 690pa 1450rpm 15kw 93db(B)","个",1]
[303,"消防高温排烟风机","32297m3/h 668pa 1450rpm 11kw 90db(B)","个",1]
[304,"消防高温排烟风机","15712m3/h 552pa 2900rpm 5.5kw 86db(B)","个",1]
[305,"消防高温排烟风机","42960m3/h 665pa 1450rpm 11kw 93db(B)","个",1]
[306,"消防高温排烟风机","38200m3/h 736pa 1450rpm 7.5kw 89db(B)","个",1]
[307,"消防高温排烟风机","42900m3/h 665pa 1450rpm 11kw 90db(B)","个",1]
[308,"消声静压箱","1800*1200*1500","个",1]
[309,"消声静压箱","1800*1200*1500","个",1]
[310,"消声静压箱","1800*1200*1500","个",1]
[311,"消声静压箱","2200*1200*1500","个",1]
[312,"消声静压箱","1800*1200*1500","个",1]
[313,"消声静压箱","1400*800*1000","个",1]
[314,"消声静压箱","1600*1800*1500","个",1]
[315,"消声静压箱","2000*1200*2000","个",1]
[316,"消声静压箱","1700*800*800","个",1]
[317,"消声静压箱","3200*1500*1500","个",1]
[318,"消声静压箱","2650*1200*1500","个",1]
[319,"消声静压箱","2600*2000*1500","个",1]
[320,"消声静压箱","4000*1500*1500","个",1]
[321,"消声静压箱","2600*2000*1500","个",1]
[322,"消声静压箱","2600*2000*1500","个",1]
[323,"消声静压箱","3400*1500*1500","个",1]
[324,"消声静压箱","2200*1500*1500","个",1]
[325,"消声静压箱","1500*1200*1500","个",1]
[326,"消声静压箱","1500*1200*800","个",1]
[327,"消声静压箱","2400*2000*1000","个",1]
[328,"止回阀","1250*800","个",1,null,null,"风机进出口未知"]
[329,"止回阀","1250*1000","个",1,null,null,"风机进出口未知"]
[330,"止回阀","630*800","个",1,null,null,"风机进出口未知"]
[331,"止回阀","1250*800","个",1,null,null,"风机进出口未知"]
[332,"止回阀","1250*1000","个",1,null,null,"风机进出口未知"]
[333,"止回阀","500*320","个",1,null,null,"风机进出口未知"]
[334,"止回阀","400*250","个",1,null,null,"风机进出口未知"]
[335,"止回阀","630*800","个",1,null,null,"风机进出口未知"]
[336,"止回阀","1250*800","个",1,null,null,"风机进出口未知"]
[337,"止回阀","1250*1000","个",1,null,null,"风机进出口未知"]
[338,"止回阀","800*630","个",1,null,null,"风机进出口未知"]
[339,"止回阀","1250*800","个",1,null,null,"风机进出口未知"]
[340,"止回阀","1000*1250","个",1,null,null,"风机进出口未知"]
[341,"止回阀","1200*500  ","个",1,null,null,"风机进出口未知"]
[342,"止回阀","1250*500","个",1,null,null,"风机进出口未知"]
[343,"止回阀","1000*800","个",1,null,null,"风机进出口未知"]
[344,"止回阀","630*500","个",1,null,null,"风机进出口未知"]
[345,"止回阀","1250*1000","个",1,null,null,"风机进出口未知"]
[346,"止回阀","1250*800","个",1,null,null,"风机进出口未知"]
[347,"止回阀","630*500","个",1,null,null,"风机进出口未知"]
[348,"止回阀","630*400","个",1,null,null,"风机进出口未知"]
[349,"止回阀","1000*800","个",1]
[350,"止回阀","630*1000","个",1]
[351,"止回阀","630*400","个",1]
[352,"轴流风机","18908m3/h 728pa 1450rpm 7.5kw 88db(B)","个",1]
[353,"轴流风机","22439m3/h 655pa 1450rpm 7.5kw 88db(B)","个",1]
[354,"阻抗复合型消声器","1000*1250","个",1,null,null,"长度1500"]
[355,"阻抗复合型消声器","630*800","个",1,null,null,"长度1000"]
[356,"阻抗复合型消声器","1500*630","个",1,null,null,"长度1500"]
[357,"阻抗复合型消声器","1000*1250","个",1,null,null,"长度1500"]
[358,"阻抗复合型消声器","1500*630","个",1,null,null,"长度1500"]
[359,"阻抗复合型消声器","500*320","个",2,null,null,"长度1000"]
[360,"阻抗复合型消声器","400*250","个",1,null,null,"长度1000"]
[361,"阻抗复合型消声器","630*800","个",1,null,null,"长度1000"]
[362,"阻抗复合型消声器","1000*1250","个",1,null,null,"长度1500"]
[363,"阻抗复合型消声器","630*800","个",1,null,null,"长度1000"]
[364,"阻抗复合型消声器","1500*630","个",1,null,null,"长度1500"]
[365,"阻抗复合型消声器","1000*1250","个",1,null,null,"长度1500"]
[366,"阻抗复合型消声器","1500*630","个",1,null,null,"长度1500"]
[367,"阻抗复合型消声器","1000*630","个",1,null,null,"长度1000"]
[368,"阻抗复合型消声器","1200*500","个",1,null,null,"长度1000"]
[369,"阻抗复合型消声器","1000*630","个",1,null,null,"长度1000"]
[370,"阻抗复合型消声器"," 1000*800","个",1,null,null,"长度1500"]
[371,"阻抗复合型消声器","1250*500","个",1,null,null,"长度1500"]
[372,"阻抗复合型消声器","1000*800","个",1,null,null,"长度1500"]
[373,"阻抗复合型消声器","1250*500","个",1,null,null,"长度1500"]
[374,"阻抗复合型消声器","630*500","个",1,null,null,"长度1000"]
[375,"阻抗复合型消声器","800*400","个",1,null,null,"长度1000"]
[376,"阻抗复合型消声器","1000*1250","个",1,null,null,"长度1500"]
[377,"阻抗复合型消声器","500*630","个",1,null,null,"长度1000"]
[378,"阻抗复合型消声器","1500*500","个",1]
[379,"阻抗复合型消声器","400*630","个",1,null,null,"长度1000"]
[380,"阻抗复合型消声器","800*320","个",1,null,null,"长度1000"]
[381,"阻抗复合型消声器","630*400","个",2,null,null,"长度1000"]
[382,"阻抗复合型消声器","1000*1000","个",1]
[383,"阻抗复合型消声器","2000*630","个",1]
[384,"阻抗复合型消声器","1400*800","个",1]
[385,"阻抗复合型消声器","2000*630","个",1]
[386,"阻抗复合型消声器","1500*800","个",1]
[387,"阻抗复合型消声器","2000*630","个",1]
[388,"阻抗复合型消声器","1800*630","个",1]
[389,"阻抗复合型消声器","2000*630","个",1]
[390,"阻抗复合型消声器","1400*800","个",1]
[391,"阻抗复合型消声器","2000*630","个",1]
[392,"阻抗复合型消声器","1250*800","个",1]
[393,"阻抗复合型消声器","2000*630","个",1]
[394,"阻抗复合型消声器","800*320","个",1,null,null,"长度1000"]
[395,"阻抗复合型消声器","630*400","个",1,null,null,"长度1000"]
[396,"阻抗复合型消声器","1000*500","个",1,null,null,"长度1500"]
[397,"阻抗复合型消声器","800*400","个",1,null,null,"长度1000"]
[398,"阻抗复合型消声器","630*500","个",1,null,null,"长度1000"]
[399,"阻抗复合型消声器","630*400","个",2,null,null,"长度1000"]
[400,"阻抗复合型消声器","1250*630","个",1]
[401,"阻抗复合型消声器","1800*630","个",1]
[402,"阻抗复合型消声器","630*400","个",1,null,null,"长度1500"]
[null,"游泳馆",null,"个"]
[1,"70°防火阀","800*400","个",2,null,null,"70°熔断关闭"]
[2,"70°防火阀","1250*500","个",2]
[3,"70°防火阀","1000*400","个",3,null,null,"70°熔断关闭"]
[4,"70°防火阀","320*160","个",3,null,null,"常开70°熔断关闭"]
[5,"70°防火阀","800*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[6,"70°防火阀","500*250","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[7,"70°防火阀","630*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[8,"70°防火阀","630*320","个",2,null,null,"常开70°熔断关闭"]
[9,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[10,"70°防火阀","1250*400","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[11,"70°防火阀","1000*400","个",2,null,null,"常开70°熔断关闭"]
[12,"70°防火阀","800*320","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[13,"70°防火阀","500*250","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[14,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[15,"70°防火阀","320*400","个",2,null,null,"常开70°熔断关闭"]
[16,"70°防火阀","500*320","个",2,null,null,"常开70°熔断关闭"]
[17,"70°防火阀","800*400","个",3,null,null,"常开70°熔断关闭"]
[18,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[19,"70°防火阀","500*250","个",1,null,null,"常开70°熔断关闭"]
[20,"70°防火阀","400*400","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[21,"70°防火阀","1250*800","个",1,null,null,"常开70°熔断关闭"]
[22,"70°防火阀","500*250","个",3,null,null,"常开70°熔断关闭"]
[23,"70°防火阀","630*400","个",3,null,null,"常开70°熔断关闭"]
[24,"70°防火阀","400*250","个",1,null,null,"常开70°熔断关闭"]
[25,"70°防火阀","400*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[26,"70°防火阀","400*200","个",1,null,null,"常开70°熔断关闭"]
[27,"70°防火阀","400*120","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[28,"70°防火阀","1000*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[29,"70°防火阀","500*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[30,"70°防火阀","500*250","个",2,null,null,"常开70°熔断关闭"]
[31,"70°防火阀","630*400","个",3,null,null,"常开70°熔断关闭"]
[32,"70°防火阀","320*400","个",1,null,null,"常开70°熔断关闭"]
[33,"70°防火阀","320*320","个",2,null,null,"常开70°熔断关闭"]
[34,"70°防火阀","320*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[35,"70°防火阀","630*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[36,"70°防火阀","630*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[37,"70°防火阀","1000*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[38,"70°防火阀","1000*320","个",1,null,null,"常开70°熔断关闭 "]
[39,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 "]
[40,"70°防火阀","500*250","个",2,null,null,"常开70°熔断关闭 "]
[41,"70°防火阀","1600*1000","个",1]
[42,"70°防火阀","2000*800","个",1,null,null,"常开70°熔断关闭 "]
[43,"70°防火阀","2000*500","个",4,null,null,"常开70°熔断关闭 "]
[44,"70°防火阀","1000*320","个",1,null,null,"常开70°熔断关闭 "]
[45,"70°防火阀","630*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[46,"70°防火阀","2000*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[47,"70°防火阀","1000*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[48,"70°防火阀","800*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[49,"70°防火阀","500*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[50,"70°防火阀","500*250","个",1,null,null,"常开70°熔断关闭 "]
[51,"70°防火阀","500*250","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[52,"70°防火阀","500*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[53,"70°防火阀","630*250","个",2,null,null,"常开70°熔断关闭 "]
[54,"70°防火阀","630*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[55,"70°防火阀","500*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[56,"70°防火阀","500*250","个",3,null,null,"常开70°熔断关闭 "]
[57,"70°防火阀","500*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[58,"70°防火阀","400*200","个",1,null,null,"常开70°熔断关闭 "]
[59,"70°防火阀","250*200","个",1,null,null,"常开70°熔断关闭 "]
[60,"70°防火阀","1250*400","个",3,null,null,"常开70°熔断关闭 带风量调节"]
[61,"70°防火阀","1250*400","个",3,null,null,"常开70°熔断关闭 "]
[62,"70°防火阀","1000*1000","个",1,null,null,"常开70°熔断关闭 嵌入式"]
[63,"70°防火阀","1250*500","个",3,null,null,"常开70°熔断关闭 "]
[64,"70°防火阀","800*500","个",3,null,null,"常开70°熔断关闭 "]
[65,"70°防火阀","500*500","个",1,null,null,"常开70°熔断关闭 "]
[66,"70°防火阀","1250*500","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[67,"70°防火阀","800*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[68,"70°防火阀","500*500","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[69,"70°防火阀","1200*1500","个",1,null,null,"常开70°熔断关闭 "]
[70,"70°防火阀","1250*1000","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[71,"70°防火阀","1000*630","个",2,null,null,"常开70°熔断关闭 "]
[72,"70°防火阀","630*630","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[73,"70°防火阀","630*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[74,"70°防火阀","630*630","个",2,null,null,"常开70°熔断关闭 "]
[75,"70°防火阀","630*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[76,"70°防火阀","400*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[77,"70°防火阀","400*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[78,"70°防火阀","630*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[79,"70°防火阀","1250*500","个",4,null,null,"常开70°熔断关闭 "]
[80,"70°防火阀","1000*2000","个",1]
[81,"70°防火阀","2000*630","个",1,null,null,"常开70°熔断关闭 "]
[82,"70°防火阀","800*250","个",13,null,null,"常开70°熔断关闭 带风量调节"]
[83,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[84,"70°防火阀","1250*630","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[85,"70°防火阀","800*320","个",1,null,null,"常开70°熔断关闭 "]
[86,"70°防火阀","800*320","个",5,null,null,"常开70°熔断关闭 带风量调节"]
[87,"70°防火阀","1600*800","个",2,null,null,"常开70°熔断关闭 "]
[88,"70°防火阀","1600*500","个",2,null,null,"常开70°熔断关闭 "]
[89,"70°防火阀","500*250","个",3,null,null,"常开70°熔断关闭 "]
[90,"70°防火阀","500*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[91,"70°防火阀","2000*630","个",1,null,null,"常开70°熔断关闭 "]
[92,"70°防火阀","1000*320","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[93,"70°防火阀","1000*630","个",1,null,null,"常开70°熔断关闭 "]
[94,"70°防火阀","1250*500","个",1,null,null,"常开70°熔断关闭 "]
[95,"70°防火阀","1000*320","个",3,null,null,"常开70°熔断关闭 带风量调节"]
[96,"70°防火阀","1250*320","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[97,"70°防火阀","1000*320","个",1,null,null,"常开70°熔断关闭 "]
[98,"70°防火阀","1250*500","个",4,null,null,"常开70°熔断关闭 "]
[99,"70°防火阀","1250*500","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[100,"70°防火阀","1250*500","个",2,null,null,"常开70°熔断关闭 "]
[101,"70°防火阀","1250*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[102,"70°防火阀","1000*1000","个",1,null,null,"常开70°熔断关闭 "]
[103,"70°防火阀","630*630","个",2,null,null,"常开70°熔断关闭 "]
[104,"70°防火阀","630*630","个",8,null,null,"常开70°熔断关闭 带风量调节"]
[105,"70°防火阀","1000*2000","个",1,null,null,"常开70°熔断关闭 "]
[106,"70°防火阀","1250*500","个",2,null,null,"常开70°熔断关闭 "]
[107,"70°防火阀","1250*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[108,"70°防火阀","1000*2000","个",1,null,null,"常开70°熔断关闭 "]
[109,"70°防火阀","1000*800","个",2,null,null,"常开70°熔断关闭 "]
[110,"70°防火阀","630*630","个",3,null,null,"常开70°熔断关闭 "]
[111,"70°防火阀","630*630","个",3,null,null,"常开70°熔断关闭 带风量调节"]
[112,"70°防火阀","500*500","个",1,null,null,"常开70°熔断关闭 "]
[113,"70°防火阀","500*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[114,"70°防火阀","500*250","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[115,"70°防火阀","1250*500","个",3,null,null,"常开70°熔断关闭 "]
[116,"70°防火阀","1250*500","个",2,null,null,"常开70°熔断关闭 带风量调节"]
[117,"70°防火阀","1200*1500","个",1,null,null,"常开70°熔断关闭 "]
[118,"70°防火阀","1250*630","个",1,null,null,"常开70°熔断关闭 "]
[119,"70°防火阀","1250*630","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[120,"70°防火阀","1250*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[121,"70°防火阀","800*250","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[122,"70°防火阀","1600*400","个",3,null,null,"常开70°熔断关闭 "]
[123,"70°防火阀","1600*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[124,"70°防火阀","500*320","个",4,null,null,"常开70°熔断关闭 带风量调节"]
[125,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[126,"70°防火阀","630*400","个",3,null,null,"常开70°熔断关闭 "]
[127,"70°防火阀","630*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[128,"70°防火阀","800*400","个",2,null,null,"常开70°熔断关闭 "]
[129,"70°防火阀","200*120","个",1,null,null,"常开70°熔断关闭 "]
[130,"70°防火阀","320*160","个",1,null,null,"常开70°熔断关闭 "]
[131,"70°防火阀","630*320","个",1,null,null,"常开70°熔断关闭 "]
[132,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 "]
[133,"70°防火阀","800*250","个",1,null,null,"常开70°熔断关闭 "]
[134,"70°防火阀","1000*400","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[135,"70°防火阀","2000*2000","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[136,"70°防火阀","2000*2000","个",1,null,null,"常开70°熔断关闭 "]
[137,"70°防火阀","800*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[138,"70°防火阀","630*400","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[139,"70°防火阀","3000*1500","个",3,null,null,"常开70°熔断关闭 带返回信号"]
[140,"70°防火调节阀","800*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[141,"70°防火调节阀","800*250","个",1,null,null,"常开70°熔断关闭 带风量调节 "]
[142,"70°防火调节阀","800*320","个",1,null,null,"常开70°熔断关闭 带风量调节 "]
[143,"70°防火调节阀","500*320","个",1,null,null,"常开70°熔断关闭 带风量调节 "]
[144,"单层百叶风口","600*800","个",2]
[145,"单层百叶风口","300*300","个",8,null,null,"带调节阀"]
[146,"单层百叶风口","1000*1000","个",1]
[147,"单层百叶风口","1200*1500","个",1]
[148,"单层百叶风口","1000*2000","个",1]
[149,"单层百叶风口","800*500","个",4]
[150,"单层百叶风口","1000*2000","个",1]
[151,"单层百叶风口","1000*2000","个",1]
[152,"单层百叶风口","1200*1500","个",1,null,null,"叶片水平"]
[153,"单层百叶风口","400*150","个",1]
[154,"单层百叶风口","500*250","个",1]
[155,"单层百叶风口","400*150","个",4]
[156,"单层百叶风口","150*150","个",2]
[157,"单层百叶风口","400*200","个",1]
[158,"单层百叶风口","400*150","个",6]
[159,"单层百叶风口","600*1000","个",2,null,null,"叶片水平"]
[160,"单层百叶风口","600*500","个",6,null,null,"叶片水平"]
[161,"单层百叶风口","400*200","个",1]
[162,"单层百叶风口","150*150","个",9]
[163,"单层百叶风口","7500*2000","个",1]
[164,"蛋格型风口","600*500","个",4,null,null,"带调节阀"]
[165,"蛋格型风口","300*300","个",12,null,null,"带调节阀"]
[166,"蛋格型风口","400*400","个",10,null,null,"带调节阀"]
[167,"蛋格型风口","300*300","个",16,null,null,"带调节阀"]
[168,"蛋格型风口","400*400","个",9,null,null,"带调节阀"]
[169,"蛋格型风口","250*250","个",2,null,null,"带调节阀"]
[170,"蛋格型风口","300*300","个",8,null,null,"带调节阀"]
[171,"蛋格型风口","400*400","个",6,null,null,"带调节阀"]
[172,"蛋格型风口","300*300","个",6,null,null,"带调节阀"]
[173,"蛋格型风口","800*1000","个",1]
[174,"蛋格型风口","400*400","个",6,null,null,"带调节阀"]
[175,"蛋格型风口","300*300","个",3,null,null,"带调节阀"]
[176,"蛋格型风口","250*250","个",2,null,null,"带调节阀"]
[177,"蛋格型风口","400*400","个",8,null,null,"带调节阀"]
[178,"蛋格型风口","300*300","个",3,null,null,"带调节阀"]
[179,"蛋格型风口","300*300","个",12,null,null,"带调节阀"]
[180,"蛋格型风口","600*800","个",2]
[181,"蛋格型风口","400*400","个",3,null,null,"带调节阀"]
[182,"蛋格型风口","250*250","个",12,null,null,"带调节阀"]
[183,"蛋格型风口","200*200","个",2,null,null,"带调节阀"]
[184,"蛋格型风口","800*600","个",5]
[185,"蛋格型风口","400*400","个",17,null,null,"带调节阀"]
[186,"蛋格型风口","250*250","个",2,null,null,"带调节阀"]
[187,"蛋格型风口","800*400","个",1,null,null,"带调节阀"]
[188,"蛋格型风口","400*400","个",4,null,null,"带调节阀"]
[189,"蛋格型风口","400*400","个",3,null,null,"带调节阀"]
[190,"蛋格型风口","250*250","个",2,null,null,"带调节阀"]
[191,"蛋格型风口","400*400","个",3,null,null,"带调节阀"]
[192,"蛋格型风口","250*250","个",4,null,null,"带调节阀"]
[193,"蛋格型风口","600*800","个",2]
[194,"蛋格型风口","400*400","个",17,null,null,"带调节阀"]
[195,"蛋格型风口","800*600","个",1]
[196,"蛋格型风口","1000*600","个",1]
[197,"蛋格型风口","200*200","个",34]
[198,"蛋格型风口","400*400","个",2]
[199,"蛋格型风口","300*300","个",3,null,null,"带调节阀"]
[200,"蛋格型风口","400*400","个",6,null,null,"带调节阀"]
[201,"蛋格型风口","400*400","个",9,null,null,"带调节阀"]
[202,"蛋格型风口","300*300","个",3,null,null,"带调节阀"]
[203,"蛋格型风口","400*400","个",4,null,null,"带调节阀"]
[204,"蛋格型风口","600*200","个",41,null,null,"带调节阀"]
[205,"蛋格型风口","600*200","个",45,null,null,"带调节阀"]
[206,"蛋格型风口","600*200","个",42,null,null,"带调节阀"]
[207,"蛋格型风口","200*200","个",3,null,null,"带调节阀"]
[208,"蛋格型风口","200*200","个",13,null,null,"带调节阀"]
[209,"蛋格型风口","300*300","个",8,null,null,"带调节阀"]
[210,"蛋格型风口","200*100","个",2,null,null,"带调节阀"]
[211,"蛋格型风口","600*800","个",8,null,null,"带调节阀"]
[212,"蛋格型风口","400*400","个",17,null,null,"带调节阀"]
[213,"蛋格型风口","300*500","个",1,null,null,"带调节阀"]
[214,"蛋格型风口","200*200","个",11,null,null,"带调节阀"]
[215,"蛋格型风口","200*200","个",6,null,null,"带调节阀"]
[216,"蛋格型风口","600*500","个",18,null,null,"带调节阀"]
[217,"蛋格型风口","800*600","个",1,null,null,"带调节阀"]
[218,"蛋格型风口","600*600","个",2,null,null,"带调节阀"]
[219,"蛋格型风口","600*1000","个",1,null,null,"带调节阀"]
[220,"蛋格型风口","200*200","个",20,null,null,"带调节阀"]
[221,"蛋格型风口","600*500","个",12,null,null,"带调节阀"]
[222,"蛋格型风口","1000*1000","个",4,null,null,"带调节阀"]
[223,"蛋格型风口","1000*1000","个",2,null,null,"带调节阀"]
[224,"蛋格型风口","1000*1000","个",4,null,null,"带调节阀"]
[225,"蛋格型风口","1000*1000","个",4,null,null,"带调节阀"]
[226,"蛋格型风口","300*300","个",20,null,null,"带调节阀"]
[227,"蛋格型风口","1000*1000","个",5,null,null,"带调节阀"]
[228,"蛋格型风口","1200*1000","个",3,null,null,"带调节阀"]
[229,"蛋格型风口","1000*1000","个",4,null,null,"带调节阀"]
[230,"蛋格型风口","1000*1000","个",5,null,null,"带调节阀"]
[231,"蛋格型风口","1200*1000","个",3,null,null,"带调节阀"]
[232,"蛋格型风口","800*500","个",3,null,null,"带调节阀"]
[233,"蛋格型风口","400*400","个",5,null,null,"带调节阀"]
[234,"蛋格型风口","400*600","个",3,null,null,"带调节阀"]
[235,"蛋格型风口","800*1000","个",1]
[236,"蛋格型风口","800*800","个",4,null,null,"带调节阀"]
[237,"蛋格型风口","800*800","个",4,null,null,"带调节阀"]
[238,"蛋格型风口","800*800","个",4,null,null,"带调节阀"]
[239,"蛋格型风口","1000*1000","个",9,null,null,"带调节阀"]
[240,"蛋格型风口","800*800","个",15,null,null,"带调节阀"]
[241,"蛋格型风口","1200*400","个",1]
[242,"蛋格型风口","600*600","个",2,null,null,"带调节阀"]
[243,"低噪声离心轴流风机","200m3/h 120pa 100w 44db(B)","个",1]
[244,"低燥声离心管道风机","800m3/h 156pa 800rpm 100w 61db(B)","个",1]
[245,"低燥声离心管道风机","2599m3/h 214pa  450w 60db(B)","个",1]
[246,"低燥声离心管道风机","180m3/h 132pa  100w 44db(B)","个",1]
[247,"低燥声离心管道风机","450m3/h 100pa  100w 46db(B)","个",1]
[248,"低燥声离心管道风机","180m3/h 132pa  100w 44db(B)","个",2]
[249,"低燥声离心管道风机","210m3/h 136pa  100w 46db(B)","个",1]
[250,"低燥声离心管道风机","360m3/h 142pa  100w 46db(B)","个",1]
[251,"低燥声离心管道风机","320m3/h 120pa  100w 46db(B)","个",1]
[252,"低燥声离心管道风机","120m3/h 100pa  50w 44db(B)","个",1]
[253,"低燥声离心管道风机","240m3/h 110pa  100w 44db(B)","个",2]
[254,"低燥声离心管道风机","200m3/h 20pa  100w 44db(B)","个",3]
[255,"低燥声离心管道风机","1050m3/h 138pa  100w 44db(B)","个",1]
[256,"低燥声离心管道风机","1300m3/h 220pa静195pa 900rpm 0.18kw 58db(B)","个",4]
[257,"低燥声离心管道风机","1260m3/h 100pa 100w 52db(B)","个",1]
[258,"电动双位阀","500*500","个",1]
[259,"电动双位阀","500*400","个",1]
[260,"电动双位阀","500*400","个",1]
[261,"电动双位阀","1500*1000","个",1]
[262,"电动双位阀","1600*1000","个",1]
[263,"电动双位阀","500*200","个",1]
[264,"电动双位阀","1250*1000","个",1]
[265,"电动双位阀","1800*630","个",2]
[266,"电动双位阀","800*630","个",1]
[267,"电动双位阀","1250*1000","个",2]
[268,"电动调节阀","1250*400","个",2]
[269,"电动调节阀","1250*500","个",1]
[270,"电动调节阀","1000*630","个",2]
[271,"电动调节阀","1250*500","个",1]
[272,"电动调节阀","800*800","个",1]
[273,"电动调节阀","1250*630","个",1]
[274,"电动调节阀","1250*500","个",2]
[275,"电动调节阀","1250*630","个",1]
[276,"电动调节阀","1250*500","个",2]
[277,"电动调节阀","630*800","个",1]
[278,"电动调节阀","1000*800","个",1]
[279,"电动调节阀","800*800","个",1]
[280,"多叶排烟口","1000*600","个",1,null,null,"远程手动及信号开启"]
[281,"防火阀","2000*500","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[282,"防火阀","800*630","个",2,null,null,"常开70°熔断关闭 带返回信号"]
[283,"防火阀","800*630","个",2,null,null,"常开70°熔断关闭 带返回信号"]
[284,"防火阀","1000*500","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[285,"防火阀","630*500","个",2,null,null,"常开70°熔断关闭 带返回信号"]
[286,"防火阀","1000*500","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[287,"防火风口","1800*800","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[288,"防火风口","800*1000","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[289,"防火风口","800*1000","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[290,"防烟防火阀","1250*400","个",1,null,null,"常开70°熔断关闭 带返回信号"]
[291,"防烟防火风口","400*400","个",2,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[292,"防烟防火风口","300*300","个",5,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[293,"防烟防火风口","400*400","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[294,"防烟防火调节阀","1250*400","个",1,null,null,"常开70°熔断关闭带风量调节带返回信号"]
[295,"防烟防火调节阀","1000*400","个",1,null,null,"常开70°熔断关闭带风量调节带返回信号"]
[296,"防烟防火调节阀","500*250","个",1,null,null,"常开70°熔断关闭 带风量调节 带返回信号"]
[297,"防烟防火调节阀","800*400","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[298,"防烟防火调节阀","500*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[299,"防烟防火调节阀","630*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[300,"防烟防火调节阀","500*250","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[301,"防烟防火调节阀","800*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[302,"防烟防火调节阀","1000*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[303,"防烟防火调节阀","800*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[304,"防烟防火调节阀","630*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[305,"防烟防火调节阀","630*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[306,"防烟防火调节阀","800*400","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[307,"防烟防火调节阀","500*500","个",2,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[308,"防烟防火调节阀","800*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[309,"防烟防火调节阀","800*800","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[310,"防烟防火调节阀","800*800","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[311,"防烟防火调节阀","800*320","个",1]
[312,"防雨百叶风口","800*400","个",1]
[313,"防雨百叶风口","500*250","个",1]
[314,"管道式换气扇","200m3/h 150pa  100w 40db(B)","个",2,null,null,"带止回阀"]
[315,"柜式离心防爆风机箱","2450m3/h 291pa静245pa 1100rpm 0.75kw 60db(B)","个",1]
[316,"柜式离心风机箱","6150m3/h 427pa静329pa 1000rpm 2.2kw 63db(B)","个",1]
[317,"柜式离心风机箱","17420m3/h 403pa静380pa 700rpm 7.5kw 68db(B)","个",1]
[318,"柜式离心风机箱","13900m3/h 478pa静350pa 750rpm 5.5kw 64db(B)","个",1]
[319,"柜式离心风机箱","5550m3/h 428pa静350pa 1000rpm 2.2kw 63db(B)","个",1]
[320,"柜式离心风机箱","16250m3/h 438pa静325pa 650rpm 5.5kw 64db(B)","个",1]
[321,"柜式离心风机箱","6150m3/h 427pa静329pa 1000rpm 2.2kw 62db(B)","个",1]
[322,"柜式离心风机箱","2520m3/h 251pa静203pa 1000rpm 0.75kw 59db(B)","个",1]
[323,"柜式离心风机箱","7730m3/h 421pa静338pa 800rpm 3kw 62db(B)","个",1]
[324,"柜式离心风机箱","3240m3/h 240pa静160pa 1000rpm 0.75kw 59db(B)","个",1]
[325,"柜式离心风机箱","16940m3/h 493pa静407pa 650rpm 7.5kw 69db(B)","个",1]
[326,"柜式离心风机箱","5500m3/h 428pa静350pa 1000rpm 2.2kw 62db(B)","个",1]
[327,"柜式离心风机箱","12230m3/h 550pa静443pa 800rpm 5.5kw 68db(B)","个",1]
[328,"柜式离心风机箱","5910m3/h 409pa静360pa 800rpm 3kw 62db(B)","个",1]
[329,"柜式离心风机箱","2160m3/h 240pa静205pa1000rpm 0.75kw 60db(B)","个",1]
[330,"柜式离心风机箱","4500m3/h 351pa静250pa1100rpm 1.5kw 61db(B)","个",1]
[331,"柜式离心风机箱","2160m3/h 240pa静205pa1000rpm  59db(B)","个",1]
[332,"柜式离心风机箱","8660m3/h 429pa静325pa 800rpm 3kw 62db(B)","个",1]
[333,"柜式离心风机箱","9100m3/h 418pa静360pa 700rpm 4kw 63db(B)","个",1]
[334,"柜式离心风机箱","16250m3/h 438pa静325pa 650rpm 5.5kw 68db(B)","个",1]
[335,"柜式离心风机箱","7150m3/h 471pa静400pa 850rpm 3kw 63db(B)","个",1]
[336,"柜式离心风机箱","19780m3/h 558pa 1450rpm 5.5kw ","个",1]
[337,"柜式离心风机箱","6750m3/h 321pa静258pa 700rpm 2.2kw 61db(B)","个",1]
[338,"柜式离心风机箱","11700m3/h 424pa静328pa 700rpm 4kw 63db(B)","个",1]
[339,"柜式离心风机箱","2450m3/h 291pa静245pa 1100rpm 0.75kw 60db(B)","个",1]
[340,"柜式离心风机箱","5490m3/h 520pa静444pa 1100rpm 3kw 63db(B)","个",1]
[341,"柜式离心风机箱","6000m3/h 318pa静268pa 700rpm 2.2kw 61db(B)","个",1]
[342,"柜式离心风机箱","5910m3/h 409pa静360pa 800rpm 3kw 62db(B)","个",1]
[343,"联箱","1800*1600*1500","个",1]
[344,"联箱","2000*500*2200","个",1]
[345,"联箱","1500*1500*1000","个",1]
[346,"联箱","1500*700*500","个",1]
[347,"联箱","1500*1200*2000","个",1]
[348,"联箱","1200*1200*1000","个",1]
[349,"联箱","5800*600*350","个",1]
[350,"联箱","3500*600*350","个",2]
[351,"联箱","2000*1500*600","个",1]
[352,"联箱","2500*2000*800","个",1]
[353,"联箱","1700*1200*1000","个",1]
[354,"联箱","2000*1600*1200","个",2]
[355,"联箱","1700*400*350","个",14]
[356,"联箱","1700*400*350","个",14]
[357,"联箱","2000*2000*1000","个",1]
[358,"联箱","2500*2800*800","个",1]
[359,"联箱","2000*1600*1500","个",1]
[360,"联箱","1700*400*350","个",5]
[361,"联箱","1700*400*350","个",7]
[362,"联箱","2800*1000*1500","个",1]
[363,"联箱","1500*2200*1000","个",1]
[364,"联箱","1800*2200*1000","个",1]
[365,"联箱","2150*4000*1600","个",1]
[366,"联箱","4200*900*800","个",1]
[367,"排烟阀","800*320","个",2,null,null,"常闭 信号开启及远程手动"]
[368,"排烟阀","800*320","个",2,null,null,"常闭 信号返回 远程手动"]
[369,"排烟阀","800*600","个",3,null,null,"常闭 信号返回 远程手动"]
[370,"排烟阀","800*320","个",2,null,null,"常闭 信号返回 远程手动"]
[371,"排烟阀","800*320","个",2,null,null,"常闭 信号返回 远程手动"]
[372,"排烟阀","600*800","个",1,null,null,"常闭 信号返回 远程手动"]
[373,"排烟阀","800*400","个",4,null,null,"常闭 信号返回 远程手动"]
[374,"排烟阀","800*320","个",5,null,null,"常闭 信号返回 远程手动"]
[375,"排烟阀","1250*320","个",4,null,null,"常闭 信号返回 远程手动"]
[376,"排烟阀","800*320","个",11,null,null,"常闭 信号返回 远程手动"]
[377,"排烟阀","800*400","个",1,null,null,"常闭 信号返回 远程手动"]
[378,"排烟阀","800*320","个",5,null,null,"常闭 信号返回 远程手动"]
[379,"排烟阀","630*400","个",1,null,null,"常闭 信号返回 远程手动"]
[380,"排烟阀","1000*320","个",1,null,null,"常闭 信号返回 远程手动"]
[381,"排烟防火阀","1250*400","个",6,null,null,"常开280°熔断关闭 带返回信号"]
[382,"排烟防火阀","800*320","个",2,null,null,"常开280°熔断关闭"]
[383,"排烟防火阀","φ910","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[384,"排烟防火阀","800*320","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[385,"排烟防火阀","800*630","个",2,null,null,"常开280°熔断关闭 带返回信号"]
[386,"排烟防火阀","800*600","个",3,null,null,"常开 280°熔断关闭 返回信号"]
[387,"排烟防火阀","800*320","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[388,"排烟防火阀","800*320","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[389,"排烟防火阀","1000*500","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[390,"排烟防火阀","600*800","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[391,"排烟防火阀","1000*630","个",1,null,null,"常开280°熔断关闭 带返回信号"]
[392,"排烟防火阀","1000*630","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[393,"排烟防火阀","800*400","个",5,null,null,"常开 280°熔断关闭 返回信号"]
[394,"排烟防火阀","1000*400","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[395,"排烟防火阀","800*320","个",5,null,null,"常开 280°熔断关闭 返回信号"]
[396,"排烟防火阀","2000*500","个",3,null,null,"常开280°熔断关闭 带返回信号"]
[397,"排烟防火阀","1250*320","个",4,null,null,"常开 280°熔断关闭 返回信号"]
[398,"排烟防火阀","1000*800","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[399,"排烟防火阀","1250*500","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[400,"排烟防火阀","800*320","个",11,null,null,"常开 280°熔断关闭 返回信号"]
[401,"排烟防火阀","800*400","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[402,"排烟防火阀","1000*1000","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[403,"排烟防火阀","1250*500","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[404,"排烟防火阀","800*320","个",5,null,null,"常开 280°熔断关闭 返回信号"]
[405,"排烟防火阀","630*400","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[406,"排烟防火阀","1200*1200","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[407,"排烟防火阀","1200*1200","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[408,"排烟防火阀","1000*630","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[409,"排烟防火阀","1200*1200","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[410,"排烟防火阀","1200*1200","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[411,"排烟防火阀","1000*630","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[412,"排烟防火阀","1000*320","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[413,"排烟防火阀","1000*320","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[414,"排烟防火阀","1200*1200","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[415,"排烟防火阀","1200*1200","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[416,"排烟防火阀","1200*1200","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[417,"排烟防火阀","1600*1200","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[418,"排烟防火阀","1200*1200","个",6,null,null,"常开 280°熔断关闭 返回信号"]
[419,"片式消声器","500*250","个",1,null,null,"长度1000"]
[420,"片式消声器","630*400","个",1,null,null,"长度1000"]
[421,"片式消声器","800*630","个",1,null,null,"长度1500"]
[422,"片式消声器","1000*320","个",1,null,null,"长度1000"]
[423,"片式消声器","630*400","个",1,null,null,"长度1000"]
[424,"片式消声器","1250*1250","个",1,null,null,"长度1500"]
[425,"片式消声器","800*630","个",1,null,null,"长度1500"]
[426,"片式消声器","1000*630","个",1,null,null,"长度1500"]
[427,"片式消声器","800*630","个",1,null,null,"长度1000"]
[428,"片式消声器","630*250","个",1,null,null,"长度1000"]
[429,"片式消声器","1000*320","个",1,null,null,"长度1500"]
[430,"片式消声器","1000*500","个",1,null,null,"长度1500"]
[431,"片式消声器","800*400","个",1,null,null,"长度1500"]
[432,"片式消声器","1600*1000","个",1,null,null,"长度2000"]
[433,"片式消声器","2000*800","个",1,null,null,"长度2000"]
[434,"片式消声器","500*400","个",1,null,null,"长度1000"]
[435,"片式消声器","630*250","个",1,null,null,"长度1000"]
[436,"片式消声器","500*250","个",1,null,null,"长度1000"]
[437,"片式消声器","1250*400","个",3,null,null,"长度1500"]
[438,"片式消声器","1250*500","个",4,null,null,"长度1500"]
[439,"片式消声器","800*500","个",4,null,null,"长度1500"]
[440,"片式消声器","1250*1000","个",1,null,null,"长度1500"]
[441,"片式消声器","630*630","个",2,null,null,"长度1000"]
[442,"片式消声器","630*400","个",1,null,null,"长度1000"]
[443,"片式消声器","800*250","个",1,null,null,"长度1000"]
[444,"片式消声器","2000*630","个",1,null,null,"长度1500"]
[445,"片式消声器","800*320","个",1,null,null,"长度1500"]
[446,"片式消声器","1600*800","个",1,null,null,"长度1500"]
[447,"片式消声器","500*250","个",1,null,null,"长度1500"]
[448,"片式消声器","2000*630","个",1,null,null,"长度2000"]
[449,"片式消声器","2000*630","个",1,null,null,"长度1000"]
[450,"片式消声器","1250*500","个",4,null,null,"长度1500"]
[451,"片式消声器","1250*500","个",1,null,null,"长度1000"]
[452,"片式消声器","1250*500","个",1,null,null,"长度1000"]
[453,"片式消声器","500*500","个",1,null,null,"长度1000"]
[454,"片式消声器","1250*500","个",2,null,null,"长度1500"]
[455,"片式消声器","1250*630","个",1,null,null,"长度2000"]
[456,"片式消声器","630*400","个",1,null,null,"长度1000"]
[457,"片式消声器","800*400","个",1,null,null,"长度1000"]
[458,"片式消声器","800*630","个",1,null,null,"长度1500"]
[459,"片式消声器","800*400","个",2,null,null,"长度1000"]
[460,"片式消声器","800*1600","个",1,null,null,"长度1500"]
[461,"片式消声器","800*1600","个",1,null,null,"长度1500"]
[462,"片式消声器","1500*1000","个",1]
[463,"双层百叶风口","1600*250","个",14,null,null,"前组叶片垂直"]
[464,"双层百叶风口","200*200","个",6]
[465,"双层百叶风口","1600*250","个",14,null,null,"前组叶片垂直"]
[466,"双层百叶风口","1600*250","个",5,null,null,"前组叶片垂直 带调节阀"]
[467,"双层百叶风口","1600*250","个",7,null,null,"前组叶片垂直"]
[468,"双层百叶风口","400*200","个",15,null,null,"前组叶片水平 带调节阀"]
[469,"双层百叶送风口","200*200","个",3,null,null,"带风量调节"]
[470,"条形散流器","400*200","个",2,null,null,"带调节阀"]
[471,"条形散流器","400*100","个",1,null,null,"带调节阀"]
[472,"条形散流器","1000*200","个",6,null,null,"带调节阀"]
[473,"条形散流器","400*150","个",16]
[474,"调节阀","400*200","个",4]
[475,"调节阀","500*250","个",4]
[476,"调节阀","500*200","个",7]
[477,"调节阀","630*250","个",3]
[478,"调节阀","800*400","个",1]
[479,"调节阀","800*320","个",2]
[480,"调节阀","500*200","个",1]
[481,"调节阀","800*250","个",2]
[482,"调节阀","500*250","个",4]
[483,"调节阀","400*400","个",2]
[484,"调节阀","500*250","个",3]
[485,"调节阀","500*200","个",1]
[486,"调节阀","400*250","个",4]
[487,"调节阀","500*250","个",2]
[488,"调节阀","500*320","个",3]
[489,"调节阀","630*200","个",6]
[490,"调节阀","500*200","个",4]
[491,"调节阀","500*250","个",3]
[492,"调节阀","500*120","个",12]
[493,"调节阀","630*250","个",1]
[494,"调节阀","500*320","个",3]
[495,"调节阀","630*250","个",4]
[496,"调节阀","500*200","个",1]
[497,"调节阀","630*200","个",1]
[498,"调节阀","800*500","个",1]
[499,"调节阀","630*400","个",4]
[500,"调节阀","200*160","个",6]
[501,"调节阀","200*120","个",1]
[502,"调节阀","200*120","个",3]
[503,"调节阀","200*160","个",5]
[504,"调节阀","200*160","个",4]
[505,"调节阀","200*120","个",2]
[506,"调节阀","500*250","个",3]
[507,"调节阀","500*200","个",4]
[508,"调节阀","500*120","个",8]
[509,"调节阀","500*400","个",1]
[510,"调节阀","400*120","个",8]
[511,"调节阀","630*400","个",1]
[512,"调节阀","500*200","个",2]
[513,"调节阀","250*200","个",3]
[514,"调节阀","200*120","个",2]
[515,"调节阀","630*320","个",3]
[516,"调节阀","500*200","个",5]
[517,"调节阀","500*250","个",1]
[518,"调节阀","500*160","个",2]
[519,"调节阀","200*160","个",8]
[520,"调节阀","200*120","个",4]
[521,"调节阀","400*120","个",12]
[522,"调节阀","500*200","个",7]
[523,"调节阀","500*320","个",1]
[524,"调节阀","400*120","个",2]
[525,"调节阀","500*320","个",3]
[526,"调节阀","500*250","个",1]
[527,"调节阀","500*160","个",3]
[528,"调节阀","500*120","个",3]
[529,"调节阀","250*160","个",1]
[530,"调节阀","200*120","个",1]
[531,"调节阀","120*120","个",2]
[532,"调节阀","630*200","个",7]
[533,"调节阀","630*120","个",1]
[534,"调节阀","400*120","个",7]
[535,"调节阀","500*250","个",4]
[536,"调节阀","320*160","个",3]
[537,"调节阀","400*120","个",2]
[538,"调节阀","400*200","个",8]
[539,"调节阀","1000*1000","个",1]
[540,"调节阀","400*120","个",4]
[541,"调节阀","400*160","个",8]
[542,"调节阀","1000*250","个",1]
[543,"调节阀","630*250","个",4]
[544,"调节阀","500*200","个",3]
[545,"调节阀","630*320","个",1]
[546,"调节阀","500*250","个",1]
[547,"调节阀","500*250","个",1]
[548,"调节阀","500*120","个",1]
[549,"调节阀","500*320","个",1]
[550,"调节阀","630*320","个",1]
[551,"调节阀","630*320","个",1]
[552,"通风消防两用双速离心柜式风机箱","33980/49640m3/h 462/1072pa静320/770pa 550/730rpm11/33kw 72db(B)","个",1]
[553,"通风消防两用双速离心柜式风机箱","25600/37700m3/h 465/1010pa静344/748pa 550/810rpm8.5/24kw 72db(B)","个",1]
[554,"通风消防两用双速离心柜式风机箱","25600/37700m3/h 465/1010pa静344/748pa 550/810rpm8.5/24kw 72db(B)","个",1]
[555,"通风消防两用双速离心柜式风机箱\n","33980/49610m3/h 462/101072pa静320/770pa 550/730rpm11/33kw 72db(B)","个",1]
[556,"通风消防两用双速离心柜式风机箱\n","33980/49610m3/h 462/101072pa静320/770pa 550/730rpm11/33kw 72db(B)","个",1]
[557,"通风消防两用双速离心柜式风机箱\n","33980/49610m3/h 462/101072pa静320/770pa 550/730rpm11/33kw 72db(B)","个",1]
[558,"消防高温排烟风机","31421m3/h 600pa 1450rpm 7.5kw ","个",1]
[559,"消防高温排烟风机","31421m3/h 600pa 1450rpm 7.5kw ","个",1]
[560,"消防高温排烟风机","38200m3/h 668pa 1450rpm 11kw ","个",1]
[561,"消防高温排烟风机","38200m3/h 668pa 1450rpm 11kw ","个",1]
[562,"消防高温排烟风机","61652m3/h 765pa 960rpm 18.5kw ","个",1]
[563,"消防高温排烟风机","38200m3/h 668pa 1450rpm 11kw ","个",1]
[564,"消防高温排烟风机","38200m3/h 668pa 1450rpm 11kw ","个",1]
[565,"消防高温排烟风机","71120m3/h 672pa 960rpm 18.5kw ","个",1]
[566,"消防高温排烟风机","71120m3/h 672pa 960rpm 18.5kw ","个",1]
[567,"消防高温排烟风机","71120m3/h 672pa 960rpm 18.5kw ","个",1]
[568,"消防高温排烟风机","71120m3/h 672pa 960rpm 18.5kw ","个",1]
[569,"消防高温排烟风机","38200m3/h 668pa 1450rpm 11kw ","个",1]
[570,"消防高温排烟风机","38200m3/h 668pa 1450rpm 11kw ","个",1]
[571,"消防高温排烟风机","18908m3/h 728pa 1450rpm 7.5kw ","个",1]
[572,"消防高温排烟轴流风机","66370m3/h 710pa 960rpm 18.5kw ","个",2]
[573,"消防高温排烟轴流风机","66370m3/h 710pa 960rpm 18.5kw ","个",3]
[574,"消防高温排烟轴流风机","32297m3/h 668pa 1450rpm 11kw ","个",1]
[575,"消防通风双速离心风机","21290/31500m3/h 388/850pa静300/662pa 500/730rpm 5.1/15.5KW 70db(B)","个",1]
[576,"消声静压箱","1000*800*800","个",1]
[577,"消声静压箱","1000*800*800","个",1]
[578,"消声静压箱","3200*1500*1200","个",1,null,null,"无机房图纸"]
[579,"消声静压箱","2500*1500*1000","个",1,null,null,"无机房图纸"]
[580,"消声静压箱","3000*2600*1000","个",1]
[581,"消声静压箱","3000*1200*1000","个",1]
[582,"消声静压箱","3000*2600*1000","个",1]
[583,"消声静压箱","3000*1200*1000","个",1]
[584,"消声静压箱","2200*2000*1000","个",1]
[585,"消声联箱","3200*1500*1500","个",2]
[586,"消声联箱","3200*1500*1500","个",2]
[587,"园盘型散流器","φ350","个",10,null,null,"带调节阀"]
[588,"园盘型散流器","φ315","个",23,null,null,"带调节阀"]
[589,"园盘型散流器","φ315","个",19,null,null,"带调节阀"]
[590,"园盘型散流器","φ315","个",27,null,null,"带调节阀"]
[591,"园盘型散流器","φ350","个",17,null,null,"带调节阀"]
[592,"止回阀","φ910","个",1,null,null,"风机进出口未知"]
[593,"止回阀","320*160","个",1]
[594,"止回阀","800*400","个",1,null,null,"风机进出口未知"]
[595,"止回阀","500*250","个",1,null,null,"风机进出口未知"]
[596,"止回阀","1250*800","个",1,null,null,"风机进出口未知"]
[597,"止回阀","φ810","个",1,null,null,"风机进出口未知"]
[598,"止回阀","φ810","个",1,null,null,"风机进出口未知"]
[599,"止回阀","500*250","个",1,null,null,"风机进出口未知"]
[600,"止回阀","500*400","个",1,null,null,"风机进出口未知"]
[601,"止回阀","800*630","个",1,null,null,"风机进出口未知"]
[602,"止回阀","800*630","个",1,null,null,"风机进出口未知"]
[603,"止回阀","500*250","个",1,null,null,"风机进出口未知"]
[604,"止回阀","630*400","个",1,null,null,"风机进出口未知"]
[605,"止回阀","400*320","个",1,null,null,"风机进出口未知"]
[606,"止回阀","1250*1250","个",1,null,null,"风机进出口未知"]
[607,"止回阀","800*630","个",1,null,null,"风机进出口未知"]
[608,"止回阀","φ910","个",1,null,null,"风机进出口未知"]
[609,"止回阀","800*630","个",1,null,null,"风机进出口未知"]
[610,"止回阀","320*160","个",1]
[611,"止回阀","320*160","个",4,null,null,"风机进出口未知"]
[612,"止回阀","320*160","个",1,null,null,"风机进出口未知"]
[613,"止回阀","1250*400","个",1,null,null,"风机进出口未知"]
[614,"止回阀","φ1210","个",1,null,null,"风机进出口未知"]
[615,"止回阀","400*200","个",1,null,null,"风机进出口未知"]
[616,"止回阀","630*320","个",1,null,null,"风机进出口未知"]
[617,"止回阀","1000*1000","个",1,null,null,"风机进出口未知"]
[618,"止回阀","1000*500","个",1,null,null,"风机进出口未知"]
[619,"止回阀","φ1310","个",1]
[620,"止回阀","φ1310","个",1]
[621,"止回阀","800*400","个",1]
[622,"止回阀","1000*400","个",1]
[623,"止回阀","1200*1200","个",1]
[624,"止回阀","1200*1200","个",1]
[625,"止回阀","1200*1200","个",1]
[626,"止回阀","1250*1250","个",2]
[627,"止回阀","1200*1200","个",3]
[628,"止回阀","320*400","个",1]
[629,"止回阀","500*320","个",1]
[630,"止回阀","320*160","个",6]
[631,"止回阀","500*200","个",1]
[632,"止回阀","800*400","个",1]
[633,"止回阀","1200*1200","个",1]
[634,"止回阀","1200*1200","个",1]
[635,"止回阀","400*160","个",3]
[636,"止回阀","320*120","个",5]
[637,"轴流风机","27600m3/h 423pa 960rpm 5.5kw 59db(B)","个",1]
[638,"轴流风机","27600m3/h 423pa 960rpm 5.5kw 59db(B)","个",1]
[639,"轴流风机","16254m3/h 702pa 1450rpm 5.5kw ","个",1]
[640,"自垂式百叶风口","350*2000","个",1]
[641,"阻抗复合型消声器","800*400","个",1,null,null,"长度1000"]
[642,"阻抗复合型消声器","1250*500","个",2]
[643,"阻抗复合型消声器","1000*500","个",2]
[644,"阻抗复合型消声器","1000*500","个",1]
[645,"阻抗复合型消声器","800*500","个",1]
[646,"阻抗复合型消声器","630*320","个",1,null,null,"长度1000"]
[647,"阻抗复合型消声器","800*400","个",1,null,null,"长度1000"]
[648,"阻抗复合型消声器","1250*400","个",1,null,null,"长度1500"]
[649,"阻抗复合型消声器","800*400","个",1]
[650,"阻抗复合型消声器","800*400","个",2]
[651,"阻抗复合型消声器","500*250","个",1,null,null,"长度1000"]
[652,"阻抗复合型消声器","1250*800","个",1,null,null,"长度1500"]
[653,"阻抗复合型消声器","500*250","个",1,null,null,"长度1000"]
[654,"阻抗复合型消声器","1000*400","个",2,null,null,"长度1500"]
[655,"阻抗复合型消声器","800*400","个",1,null,null,"长度1000"]
[656,"阻抗复合型消声器","800*250","个",1,null,null,"长度1000"]
[657,"阻抗复合型消声器","800*400","个",1,null,null,"长度1000"]
[658,"阻抗复合型消声器","1200*1200","个",1,null,null,"长度1500"]
[659,"阻抗复合型消声器","1200*1200","个",1,null,null,"长度1500"]
[660,"阻抗复合型消声器","1200*1200","个",1,null,null,"长度1500"]
[661,"阻抗复合型消声器","800*500","个",1]
[662,"阻抗复合型消声器","400*400","个",1,null,null,"长度1000"]
[663,"阻抗复合型消声器","3000*1500","个",1,null,null,"长度2000"]
[null,"健身馆",null,"个"]
[1,"150°防火阀","800*630","个",2,null,null,"常开150°熔断关闭 "]
[2,"150°防火阀","800*630","个",3,null,null,"常开150°熔断关闭 "]
[3,"150°防火阀","500*400","个",5]
[4,"150°防火阀","1000*500","个",4,null,null,"常开150°熔断关闭 "]
[5,"150°防火阀","1000*630","个",3,null,null,"常开150°熔断关闭 "]
[6,"70°防火阀","800*320","个",1,null,null,"常开70°熔断关闭 "]
[7,"70°防火阀","1000*250","个",3,null,null,"常开70°熔断关闭 "]
[8,"70°防火阀","1000*1250","个",3,null,null,"常开70°熔断关闭 带返回信号"]
[9,"70°防火阀","630*500","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[10,"70°防火阀","800*630","个",1,null,null,"常开70°熔断关闭 "]
[11,"70°防火阀","1000*500","个",1,null,null,"常开70°熔断关闭 "]
[12,"70°防火阀","1000*630","个",1,null,null,"常开70°熔断关闭 "]
[13,"70°防火阀","800*400","个",2,null,null,"常开70°熔断关闭 "]
[14,"70°防火阀","1000*400","个",1]
[15,"70°防火阀","1000*630","个",2,null,null,"常开70°熔断关闭 "]
[16,"70°防火阀","1250*630","个",2,null,null,"常开70°熔断关闭 "]
[17,"70°防火阀","630*500","个",1,null,null,"常开70°熔断关闭 "]
[18,"70°防火阀","630*400","个",1,null,null,"常开70°熔断关闭 "]
[19,"70°防火阀","1000*500","个",1,null,null,"常开70°熔断关闭 "]
[20,"70°防火阀","1000*320","个",1,null,null,"常开70°熔断关闭 "]
[21,"70°防火阀","1250*320","个",1,null,null,"常开70°熔断关闭 "]
[22,"70°防火阀","500*500","个",1,null,null,"常开70°熔断关闭 "]
[23,"70°防火阀","500*400","个",6,null,null,"常开70°熔断关闭 "]
[24,"70°防火阀","500*400","个",6,null,null,"常开70°熔断关闭 "]
[25,"70°防火阀","400*320","个",4,null,null,"常开70°熔断关闭 "]
[26,"70°防火阀","400*320","个",1,null,null,"常开70°熔断关闭 "]
[27,"70°防火阀","800*500","个",1,null,null,"常开70°熔断关闭 "]
[28,"70°防火阀","1250*630","个",3,null,null,"常开70°熔断关闭 "]
[29,"70°防火阀","1000*630","个",3,null,null,"常开70°熔断关闭 "]
[30,"70°防火阀","800*400","个",2,null,null,"常开70°熔断关闭 "]
[31,"70°防火阀","800*630","个",1,null,null,"常开70°熔断关闭 "]
[32,"70°防火阀","1400*320","个",1,null,null,"常开70°熔断关闭 "]
[33,"70°防火阀","500*320","个",2,null,null,"常开70°熔断关闭 "]
[34,"70°防火阀","500*500","个",1,null,null,"常开70°熔断关闭 "]
[35,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 "]
[36,"70°防火阀","1250*630","个",1,null,null,"常开70°熔断关闭 "]
[37,"70°防火阀","1000*630","个",1,null,null,"常开70°熔断关闭 "]
[38,"70°防火阀","800*400","个",1,null,null,"常开70°熔断关闭 "]
[39,"70°防火阀","400*320","个",3,null,null,"常开70°熔断关闭 "]
[40,"70°防火阀","320*200","个",1,null,null,"常开70°熔断关闭 "]
[41,"70°防火阀","1000*500","个",1,null,null,"常开70°熔断关闭 "]
[42,"70°防火阀","800*500","个",1,null,null,"常开70°熔断关闭 "]
[43,"70°防火阀","1600*630","个",3,null,null,"常开70°熔断关闭 "]
[44,"70°防火阀","1250*630","个",2,null,null,"常开70°熔断关闭 "]
[45,"70°防火阀","630*630","个",1,null,null,"常开70°熔断关闭 "]
[46,"70°防火阀","1250*500","个",3,null,null,"常开70°熔断关闭 "]
[47,"70°防火阀","1250*630","个",1,null,null,"常开70°熔断关闭 "]
[48,"70°防火阀","1250*500","个",2,null,null,"常开70°熔断关闭 "]
[49,"70°防火阀","1250*630","个",1,null,null,"常开70°熔断关闭 "]
[50,"70°防火阀","500*320","个",2,null,null,"常开70°熔断关闭 "]
[51,"70°防火阀","1000*630","个",1,null,null,"常开70°熔断关闭 "]
[52,"70°防火阀","1250*630","个",1,null,null,"常开70°熔断关闭 "]
[53,"70°防火阀","1600*630","个",4,null,null,"常开70°熔断关闭 "]
[54,"70°防火阀","2000*630","个",3,null,null,"常开70°熔断关闭 "]
[55,"70°防火阀","1250*800","个",2,null,null,"常开70°熔断关闭 "]
[56,"70°防火阀","1000*630","个",2,null,null,"常开70°熔断关闭 "]
[57,"70°防火阀","1250*630","个",2,null,null,"常开70°熔断关闭 "]
[58,"70°防火阀","1600*630","个",2,null,null,"常开70°熔断关闭 "]
[59,"70°防火阀","1600*630","个",4,null,null,"常开70°熔断关闭 "]
[60,"70°防火阀","1250*630","个",3,null,null,"常开70°熔断关闭 "]
[61,"单层百叶风口","1600*800","个",3,null,null,"叶片垂直"]
[62,"单层百叶风口","630*400","个",4,null,null,"叶片垂直 带调节阀"]
[63,"单层百叶风口","800*400","个",2,null,null,"叶片垂直 带调节阀"]
[64,"单层百叶风口","630*500","个",4,null,null,"叶片垂直 带调节阀"]
[65,"单层百叶风口","1600*630","个",2,null,null,"叶片垂直 带调节阀"]
[66,"单层百叶风口","1000*500","个",2,null,null,"叶片垂直 带调节阀"]
[67,"单层百叶风口","1000*630","个",1,null,null,"叶片垂直 带调节阀"]
[68,"单层百叶风口","1250*800","个",5,null,null,"叶片垂直 带调节阀"]
[69,"单层百叶风口","320*250","个",12,null,null,"叶片垂直 带调节阀"]
[70,"单层百叶风口","400*250","个",6,null,null,"叶片垂直 带调节阀"]
[71,"单层百叶风口","400*250","个",12,null,null,"叶片垂直 带调节阀"]
[72,"单层百叶风口","1000*500","个",2,null,null,"叶片垂直 带调节阀"]
[73,"单层百叶风口","1000*630","个",2,null,null,"叶片垂直 带调节阀"]
[74,"单层百叶风口","800*400","个",6,null,null,"叶片垂直 带调节阀"]
[75,"单层百叶风口","400*320","个",3]
[76,"单层百叶风口","630*250","个",4,null,null,"叶片垂直 "]
[77,"单层百叶风口","500*500","个",4,null,null,"叶片垂直 带调节阀"]
[78,"单层百叶风口","1000*500","个",2,null,null,"叶片垂直 带调节阀"]
[79,"单层百叶风口","320*200","个",18,null,null,"叶片垂直 带调节阀"]
[80,"单层百叶风口","200*160","个",1,null,null,"叶片垂直 带调节阀"]
[81,"单层百叶风口","800*400","个",2,null,null,"叶片垂直 带调节阀"]
[82,"单层百叶风口","800*400","个",2,null,null,"叶片垂直 带调节阀"]
[83,"单层百叶风口","500*200","个",2,null,null,"叶片垂直 带调节阀"]
[84,"单层百叶风口","800*320","个",2,null,null,"叶片垂直 带调节阀"]
[85,"单层百叶风口","500*320","个",2,null,null,"叶片垂直 带调节阀"]
[86,"单层百叶风口","400*200","个",7,null,null,"叶片垂直 带调节阀"]
[87,"单层百叶风口","1250*630","个",2,null,null,"叶片垂直 带调节阀"]
[88,"单层百叶风口","800*400","个",22,null,null,"叶片垂直 带调节阀"]
[89,"单层百叶风口","400*400","个",6,null,null,"叶片垂直 带调节阀"]
[90,"单层百叶风口","630*250","个",6,null,null,"叶片垂直 带调节阀"]
[91,"单层百叶风口","800*500","个",4,null,null,"叶片垂直 带调节阀"]
[92,"单层百叶风口","250*160","个",1,null,null,"叶片垂直 带调节阀"]
[93,"单层百叶风口","320*250","个",6,null,null,"叶片垂直 带调节阀"]
[94,"单层百叶风口","2000*1000","个",2,null,null,"叶片垂直 带调节阀"]
[95,"单层百叶风口","800*400","个",2,null,null,"叶片垂直 带调节阀"]
[96,"单层百叶风口","800*400","个",2,null,null,"叶片垂直 带调节阀"]
[97,"单层百叶风口","400*400","个",9,null,null,"叶片垂直 带调节阀"]
[98,"单层百叶风口","800*500","个",3,null,null,"叶片垂直 带调节阀"]
[99,"单层百叶风口","1000*630","个",3,null,null,"叶片垂直 带调节阀"]
[100,"单层百叶风口","1250*1000","个",2,null,null,"叶片垂直 带调节阀"]
[101,"单层百叶风口","160*160","个",1]
[102,"单层百叶风口","1000*800","个",3,null,null,"叶片垂直 带调节阀"]
[103,"单层百叶风口","800*500","个",3,null,null,"叶片垂直 带调节阀"]
[104,"单层百叶风口","1250*1000","个",2,null,null,"叶片垂直 带调节阀"]
[105,"单层百叶风口","160*160","个",2,null,null,"叶片垂直 带调节阀"]
[106,"单层百叶风口","1250*1000","个",2,null,null,"叶片垂直 带调节阀"]
[107,"单层百叶风口","400*250","个",4,null,null,"叶片垂直 带调节阀"]
[108,"单层百叶风口","400*200","个",2,null,null,"叶片垂直 带调节阀"]
[109,"单层百叶风口","400*400","个",10,null,null,"叶片垂直 带调节阀"]
[110,"单层百叶风口","1250*630","个",4,null,null,"叶片垂直 带调节阀"]
[111,"单层百叶风口","1250*800","个",5,null,null,"叶片垂直 带调节阀"]
[112,"单层百叶风口","1000*800","个",4,null,null,"叶片垂直 带调节阀"]
[113,"单层百叶风口","1000*800","个",4,null,null,"叶片垂直 带调节阀"]
[114,"单层百叶风口","1000*800","个",4,null,null,"叶片垂直 带调节阀"]
[115,"单层百叶风口","200*160","个",3,null,null,"叶片垂直 带调节阀"]
[116,"单层百叶风口","400*200","个",5,null,null,"叶片垂直 带调节阀"]
[117,"单层百叶风口","320*200","个",7,null,null,"叶片垂直 带调节阀"]
[118,"单层百叶风口","200*160","个",1,null,null,"叶片垂直 带调节阀"]
[119,"单层百叶风口","250*160","个",3,null,null,"叶片垂直 带调节阀"]
[120,"单层百叶风口","1000*1000","个",2,null,null,"带调节阀"]
[121,"蛋格型风口","800*200","个",6,null,null,"带调节阀"]
[122,"低燥声管道式风机","3200m3/h 185pa静145pa 550rpm 0.37kw 68db(B)","个",1]
[123,"低燥声管道式风机","1780m3/h 190pa静169pa 550rpm 0.18kw 56db(B)","个",1]
[124,"低燥声管道式风机","900m3/h 128pa静119pa 550rpm 0.12kw 52db(B)","个",1]
[125,"低燥声离心管道风机","4000m3/h 280pa静241pa 550rpm 0.65kw 63db(B)","个",1]
[126,"低燥声离心管道风机","900m3/h 128pa静119pa 550rpm 0.12kw 52db(B)","个",1]
[127,"低燥声离心管道风机","2750m3/h 250pa静221pa 550rpm 0.37kw 60db(B)","个",1]
[128,"电动双位阀","800*320","个",1]
[129,"电动双位阀","630*500","个",1]
[130,"电动双位阀","1000*500","个",1]
[131,"电动双位阀","1000*400","个",1]
[132,"电动双位阀","800*400","个",1]
[133,"电动双位阀","400*320","个",1]
[134,"电动双位阀","500*320","个",1]
[135,"电动双位阀","800*630","个",1]
[136,"电动双位阀","1000*500","个",1]
[137,"电动双位阀","800*630","个",1]
[138,"电动双位阀","800*500","个",1]
[139,"电动双位阀","500*320","个",1]
[140,"电动调节阀","800*630","个",1]
[141,"电动调节阀","800*400","个",2]
[142,"电动调节阀","1000*630","个",1]
[143,"电动调节阀","1000*500","个",1]
[144,"电动调节阀","1000*320","个",1]
[145,"电动调节阀","1000*630","个",1]
[146,"电动调节阀","1000*630","个",2]
[147,"电动调节阀","1250*630","个",2]
[148,"电动调节阀","1250*630","个",1]
[149,"电动调节阀","1600*630","个",1]
[150,"电动调节阀","1250*800","个",2]
[151,"电动调节阀","1250*630","个",2]
[152,"电动调节阀","1600*500","个",1]
[153,"电动调节阀","1600*500","个",1]
[154,"防火风口","2000*2000","个",1,null,null,"常开70°熔断关闭 "]
[155,"防火风口","3000*1600","个",1,null,null,"常开70°熔断关闭 "]
[156,"防火风口","2500*2000","个",1,null,null,"常开70°熔断关闭 "]
[157,"防火风口","2500*2000","个",1]
[158,"防火风口","1250*2500","个",2,null,null,"常开70°熔断关闭 "]
[159,"防火风口","3800*2000","个",1]
[160,"防火风口","1800*2000","个",2]
[161,"防火风口","2500*1250","个",2]
[162,"防火风口","1250*2500","个",2,null,null,"常开70°熔断关闭 "]
[163,"防烟防火阀","800*630","个",1,null,null,"常开 70°熔断关闭 返回信号"]
[164,"防烟防火阀","1000*630","个",1,null,null,"常开 70°熔断关闭 返回信号"]
[165,"防烟防火阀","1250*630","个",1,null,null,"常开 70°熔断关闭 返回信号"]
[166,"防烟防火阀","800*320","个",2,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[167,"防烟防火阀","1000*1000","个",1,null,null,"常开 70°熔断关闭 返回信号"]
[168,"防烟防火风口","200*200","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[169,"防烟防火调节阀","320*250","个",2,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[170,"防烟防火调节阀","320*200","个",2,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[171,"防烟防火调节阀","320*250","个",5,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[172,"防烟防火调节阀","1250*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[173,"防烟防火调节阀","800*320","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[174,"防烟防火调节阀","1250*500","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[175,"防烟防火调节阀","1000*500","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[176,"防烟防火调节阀","1250*500","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[177,"防烟防火调节阀","800*250","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[178,"防烟防火调节阀","1000*400","个",1,null,null,"常开70°熔断关闭 带风量调节 返回信号"]
[179,"防烟防火调节阀","800*320","个",2]
[180,"防雨百叶","4000*800","个",1]
[181,"防雨百叶风口","400*320","个",1]
[182,"防雨百叶风口","400*320","个",1]
[183,"防雨百叶风口","630*400","个",1]
[184,"防雨百叶风口","400*320","个",1]
[185,"柜式离心风机箱","18000m3/h 540pa静480pa 600rpm 11kw 67db(B)","个",1]
[186,"柜式离心风机箱","18000m3/h 540pa静480pa 600rpm 11kw 67db(B)","个",1]
[187,"柜式离心风机箱","18000m3/h 540pa静480pa 600rpm 11kw 67db(B)","个",1]
[188,"柜式离心风机箱","18000m3/h 540pa静480pa 600rpm 11kw 67db(B)","个",1]
[189,"回风箱","1400*500*500","个",3]
[190,"回风箱","1400*500*500","个",4]
[191,"回风箱","1400*500*500","个",1]
[192,"回风箱","1400*500*500","个",2]
[193,"回风箱","1250*500*400","个",1]
[194,"回风箱","1400*500*500","个",2]
[195,"回风箱","1250*500*400","个",1]
[196,"回风箱","1400*500*500","个",2]
[197,"回风箱","1250*500*400","个",1]
[198,"回风箱","1400*500*500","个",3]
[199,"回风箱","1250*500*400","个",2]
[200,"回风箱","1400*500*500","个",3]
[201,"回风箱","1400*500*500","个",1]
[202,"回风箱","1400*500*500","个",2]
[203,"回风箱","1400*500*500","个",2]
[204,"回风箱","1400*500*500","个",2]
[205,"回风箱","1400*500*500","个",2]
[206,"回风箱","1400*500*500","个",14]
[207,"回风箱","1400*500*500","个",2]
[208,"回风箱","1250*500*400","个",1]
[209,"混流风机","7187m3/h 240pa 960rpm 1.1kw ","个",1]
[210,"混流风机","5977m3/h 282pa 960rpm 1.1kw ","个",1]
[211,"混流风机","3473m3/h 341pa 1450rpm 0.75kw 60db（A） ","个",1]
[212,"混流风机","5400m3/h 198pa 960rpm 0.75kw 58db(A)","个",1]
[213,"混流风机","5400m3/h 198pa 960rpm 0.75kw 59db(A) ","个",1]
[214,"混流风机","5252m3/h 326pa 1450rpm 1.1kw 62db(A) ","个",1]
[215,"混流风机","5400m3/h 198pa静400pa 960rpm 0.75kw 59db(B)","个",1]
[216,"混流风机（防爆型）","3908m3/h 449pa 1450rpm 1.1kw 60db(A) ","个",1]
[217,"混流风机（防爆型）","3908m3/h 449pa 1450rpm 1.1kw 60db(A) ","个",1]
[218,"静压箱","3600*1000*800","个",1]
[219,"静压箱","2200*630*3000","个",1]
[220,"静压箱","2600*1500*800","个",1]
[221,"静压箱","3200*1250*800","个",1]
[222,"静压箱","3200*800*1800","个",1]
[223,"静压箱","4200*1000*1000","个",1]
[224,"静压箱","2600*800*2200","个",1]
[225,"静压箱","1000*2500*2900","个",1]
[226,"静压箱","3800*1000*1000","个",1]
[227,"静压箱","4000*1200*800","个",1]
[228,"静压箱","5500*400*4000","个",1]
[229,"可开铰链式百叶","1250*400","个",3,null,null,"带过滤网"]
[230,"可开铰链式百叶","1250*400","个",4,null,null,"带过滤网"]
[231,"可开铰链式百叶","1250*400","个",1,null,null,"带过滤网"]
[232,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[233,"可开铰链式百叶","1000*400","个",1,null,null,"带过滤网"]
[234,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[235,"可开铰链式百叶","1000*400","个",1,null,null,"带过滤网"]
[236,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[237,"可开铰链式百叶","1000*400","个",1,null,null,"带过滤网"]
[238,"可开铰链式百叶","1250*400","个",3,null,null,"带过滤网"]
[239,"可开铰链式百叶","1000*400","个",2,null,null,"带过滤网"]
[240,"可开铰链式百叶","1250*400","个",3,null,null,"带过滤网"]
[241,"可开铰链式百叶","1250*400","个",1,null,null,"带过滤网"]
[242,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[243,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[244,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[245,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[246,"可开铰链式百叶","1250*400","个",14,null,null,"带过滤网"]
[247,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[248,"可开铰链式百叶","1000*400","个",1,null,null,"带过滤网"]
[249,"排风口","1000*800","个",3]
[250,"排风口","630*400","个",3]
[251,"排风口","800*500","个",3]
[252,"排风口","1000*630","个",3]
[253,"排烟阀","630*400","个",5,null,null,"常闭 信号返回 远程手动"]
[254,"排烟阀","630*400","个",2,null,null,"常闭 信号返回 远程手动"]
[255,"排烟阀","800*400","个",1,null,null,"常闭 信号返回 远程手动"]
[256,"排烟阀","630*400","个",4,null,null,"常闭 信号返回 远程手动"]
[257,"排烟阀","500*400","个",1,null,null,"常闭 信号返回 远程手动"]
[258,"排烟阀","500*400","个",2,null,null,"常闭 信号返回 远程手动"]
[259,"排烟阀","630*400","个",7,null,null,"常闭 信号返回 远程手动"]
[260,"排烟阀","800*320","个",2,null,null,"常闭 信号返回 远程手动"]
[261,"排烟阀","500*500","个",2,null,null,"常闭 信号返回 远程手动"]
[262,"排烟阀","1250*630","个",1,null,null,"常闭 信号返回 远程手动"]
[263,"排烟阀","1000*630","个",1,null,null,"常闭 信号返回 远程手动"]
[264,"排烟阀","800*320","个",2,null,null,"常闭 信号返回 远程手动"]
[265,"排烟阀","500*500","个",3,null,null,"常闭 信号返回 远程手动"]
[266,"排烟阀","630*630","个",2,null,null,"常闭 信号返回 远程手动"]
[267,"排烟防火阀","800*630","个",4,null,null,"常开 280°熔断关闭 返回信号"]
[268,"排烟防火阀","630*400","个",5,null,null,"常开 280°熔断关闭 返回信号"]
[269,"排烟防火阀","1000*630","个",3,null,null,"常开 280°熔断关闭 返回信号"]
[270,"排烟防火阀","630*400","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[271,"排烟防火阀","800*400","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[272,"排烟防火阀","1250*1000","个",4,null,null,"常开 280°熔断关闭 返回信号"]
[273,"排烟防火阀","1250*1600","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[274,"排烟防火阀","630*400","个",4,null,null,"常开 280°熔断关闭 返回信号"]
[275,"排烟防火阀","800*630","个",5,null,null,"常开 280°熔断关闭 返回信号"]
[276,"排烟防火阀","500*400","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[277,"排烟防火阀","1000*800","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[278,"排烟防火阀","1250*630","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[279,"排烟防火阀","500*400","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[280,"排烟防火阀","630*400","个",7,null,null,"常开 280°熔断关闭 返回信号"]
[281,"排烟防火阀","800*320","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[282,"排烟防火阀","500*500","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[283,"排烟防火阀","1250*630","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[284,"排烟防火阀","1250*630","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[285,"排烟防火阀","1000*630","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[286,"排烟防火阀","800*320","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[287,"排烟防火阀","630*500","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[288,"排烟防火阀","800*800","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[289,"排烟防火阀","1000*630","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[290,"排烟防火阀","630*630","个",1]
[291,"排烟防火阀","630*400","个",1]
[292,"排烟防火阀","500*500","个",3,null,null,"常开 280°熔断关闭 返回信号"]
[293,"排烟防火阀","800*800","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[294,"排烟防火阀","630*630","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[295,"排烟防火阀","1000*1250","个",4,null,null,"常开 280°熔断关闭 返回信号"]
[296,"排烟防火阀","800*800","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[297,"排烟防火阀","1000*1250","个",6,null,null,"常开 280°熔断关闭 返回信号"]
[298,"排烟防火阀","1600*1250","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[299,"排烟防火阀","1000*1250","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[300,"排烟防火阀","1250*1000","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[301,"排烟防火阀","1250*1000","个",1,null,null,"常开 280°熔断关闭 返回信号"]
[302,"排烟防火阀","1250*800","个",2,null,null,"常开 280°熔断关闭 返回信号"]
[303,"排烟防火阀","1250*800","个",1,null,null,"常开 280°熔断关闭 返回信号 连锁关闭风机"]
[304,"片式消声器","630*500","个",2,null,null,"长度1000"]
[305,"片式消声器","630*500","个",1,null,null,"长度1000"]
[306,"片式消声器","630*400","个",1,null,null,"长度1000"]
[307,"条缝型散流器","800*200","个",50]
[308,"条缝型散流器","800*200","个",21]
[309,"条缝型散流器","1000*103","个",53]
[310,"条型散流器","800*200","个",27]
[311,"条型散流器","1000*103","个",40]
[312,"条型散流器","1000*171","个",7]
[313,"条型散流器","1000*171","个",3]
[314,"条型散流器","1000*103","个",8]
[315,"条型散流器","1000*103","个",37]
[316,"条型散流器","1000*171","个",10]
[317,"条型散流器","1000*103","个",11]
[318,"条型散流器","1000*69","个",5]
[319,"条型散流器","1000*69","个",60]
[320,"条型散流器","1000*171","个",4]
[321,"条型散流器","1000*69","个",51]
[322,"条型散流器","800*200","个",34]
[323,"条型散流器","1000*69","个",64]
[324,"条型散流器","1000*171","个",9]
[325,"条型散流器","1000*171","个",12]
[326,"条型散流器","1000*171","个",3]
[327,"条型散流器","1000*171","个",6]
[328,"条型散流器","1000*171","个",2]
[329,"条型散流器","1000*171","个",6]
[330,"条型散流器","1000*171","个",2]
[331,"条型散流器","1000*171","个",6]
[332,"条型散流器","1000*171","个",2]
[333,"条型散流器","1000*171","个",9]
[334,"条型散流器","1000*171","个",4]
[335,"条型散流器","1000*171","个",9]
[336,"条型散流器","1000*171","个",3]
[337,"条型散流器","1000*171","个",6]
[338,"条型散流器","1000*171","个",6]
[339,"条型散流器","1000*171","个",6]
[340,"条型散流器","1000*171","个",6]
[341,"条型散流器","1000*171","个",42]
[342,"条型散流器","1000*171","个",6]
[343,"条型散流器","1000*171","个",2]
[344,"条型散流器","1000*69","个",64]
[345,"调节阀","320*200","个",3]
[346,"调节阀","320*250","个",2]
[347,"调节阀","800*320","个",2]
[348,"调节阀","320*120","个",13]
[349,"调节阀","400*250","个",3]
[350,"调节阀","400*320","个",2]
[351,"调节阀","300*160","个",6]
[352,"调节阀","300*200","个",2]
[353,"调节阀","500*320","个",2]
[354,"调节阀","320*160","个",4]
[355,"调节阀","500*400","个",1]
[356,"调节阀","320*200","个",1]
[357,"调节阀","320*120","个",4]
[358,"调节阀","630*320","个",2]
[359,"调节阀","400*320","个",2]
[360,"调节阀","320*120","个",6]
[361,"调节阀","400*250","个",3]
[362,"调节阀","320*200","个",6]
[363,"调节阀","500*320","个",2]
[364,"调节阀","400*320","个",1]
[365,"调节阀","400*250","个",1]
[366,"调节阀","320*160","个",1]
[367,"调节阀","500*320","个",1]
[368,"调节阀","400*200","个",3]
[369,"调节阀","320*160","个",1]
[370,"调节阀","630*320","个",1]
[371,"调节阀","320*120","个",4]
[372,"调节阀","500*320","个",1]
[373,"调节阀","400*250","个",1]
[374,"调节阀","320*200","个",4]
[375,"调节阀","200*160","个",1]
[376,"调节阀","250*200","个",1]
[377,"调节阀","250*120","个",3]
[378,"调节阀","320*200","个",1]
[379,"调节阀","320*120","个",5]
[380,"调节阀","400*250","个",4]
[381,"调节阀","320*200","个",3]
[382,"调节阀","400*250","个",1]
[383,"调节阀","320*200","个",5]
[384,"调节阀","400*320","个",1]
[385,"调节阀","320*200","个",1]
[386,"调节阀","400*320","个",1]
[387,"调节阀","320*200","个",7]
[388,"调节阀","320*200","个",4]
[389,"调节阀","400*250","个",5]
[390,"调节阀","400*250","个",3]
[391,"调节阀","320*200","个",1]
[392,"调节阀","400*250","个",1]
[393,"调节阀","400*200","个",2]
[394,"调节阀","200*160","个",1]
[395,"调节阀","320*200","个",8]
[396,"调节阀","400*320","个",1]
[397,"调节阀","250*160","个",1]
[398,"调节阀","400*200","个",2]
[399,"调节阀","500*320","个",1,null,null,"常开70°熔断关闭 "]
[400,"调节阀","320*200","个",11,null,null,"常开70°熔断关闭 "]
[401,"调节阀","630*320","个",4,null,null,"常开70°熔断关闭 "]
[402,"调节阀","400*250","个",2,null,null,"常开70°熔断关闭 "]
[403,"调节阀","320*120","个",3,null,null,"常开70°熔断关闭 "]
[404,"调节阀","250*120","个",1]
[405,"调节阀","200*120","个",1]
[406,"调节阀","320*200","个",3]
[407,"调节阀","1000*500","个",1]
[408,"调节阀","320*200","个",9]
[409,"调节阀","400*250","个",5]
[410,"调节阀","500*400","个",1]
[411,"调节阀","500*320","个",1]
[412,"调节阀","1250*500","个",2]
[413,"调节阀","400*320","个",8]
[414,"调节阀","500*400","个",2]
[415,"调节阀","320*250","个",8]
[416,"调节阀","1000*400","个",1]
[417,"调节阀","320*200","个",6]
[418,"调节阀","400*250","个",9]
[419,"调节阀","160*120","个",1]
[420,"调节阀","400*250","个",1]
[421,"调节阀","250*160","个",1]
[422,"调节阀","250*200","个",2]
[423,"调节阀","250*120","个",1]
[424,"调节阀","200*120","个",2]
[425,"调节阀","320*250","个",4]
[426,"调节阀","320*250","个",4]
[427,"调节阀","320*250","个",1]
[428,"调节阀","320*250","个",2]
[429,"调节阀","320*250","个",1]
[430,"调节阀","320*250","个",2]
[431,"调节阀","320*250","个",2]
[432,"调节阀","320*250","个",1]
[433,"调节阀","320*250","个",5]
[434,"调节阀","320*250","个",3]
[435,"调节阀","320*250","个",1]
[436,"调节阀","320*250","个",2]
[437,"调节阀","320*250","个",4]
[438,"调节阀","320*250","个",2]
[439,"调节阀","320*250","个",2]
[440,"调节阀","320*250","个",14]
[441,"调节阀","320*200","个",2]
[442,"调节阀","320*200","个",6]
[443,"调节阀","400*250","个",9]
[444,"调节阀","1000*400","个",1]
[445,"外墙防雨百叶","1000*400","个",1]
[446,"消防轴流风机","36317m3/h 511pa 960rpm 11kw ","个",1]
[447,"消防轴流风机","38200m3/h 736pa 1450rpm 11kw ","个",1]
[448,"消防轴流风机","67845m3/h 719pa 720rpm 22kw ","个",2]
[449,"消防轴流风机","38200m3/h 736pa 1450rpm 11kw ","个",1]
[450,"消防轴流风机","40000m3/h 690pa 1450rpm 11kw ","个",1]
[451,"消防轴流风机","67845m3/h 719pa 720rpm 22kw ","个",1]
[452,"消防轴流风机","42960m3/h 665pa 1450rpm 11kw ","个",1]
[453,"消防轴流风机","18800m3/h 330pa 960rpm 3kw ","个",1]
[454,"消防轴流风机","36317m3/h 511pa 960rpm 11kw ","个",1]
[455,"消防轴流风机","42960m3/h 665pa 1450rpm 11kw ","个",1]
[456,"消防轴流风机","67845m3/h 719pa 720rpm 22kw ","个",1]
[457,"消防轴流风机","67845m3/h 719pa 720rpm 22kw ","个",2]
[458,"消防轴流风机","67845m3/h 719pa 720rpm 22kw ","个",1]
[459,"消防轴流风机","67845m3/h 719pa 720rpm 22kw ","个",1]
[460,"消防轴流风机","67845m3/h 719pa 720rpm 22kw ","个",1]
[461,"消防轴流风机","67845m3/h 719pa 720rpm 22kw ","个",1]
[462,"消声静压箱","4000*630*3000","个",1]
[463,"止回阀","1000*250","个",1]
[464,"止回阀","1000*630","个",1]
[465,"止回阀","1250*630","个",1]
[466,"止回阀","1000*630","个",1]
[467,"止回阀","1250*1000","个",2]
[468,"止回阀","630*500","个",1]
[469,"止回阀","630*500","个",1]
[470,"止回阀","1250*320","个",1]
[471,"止回阀","800*630","个",1]
[472,"止回阀","500*500","个",1]
[473,"止回阀","500*400","个",1]
[474,"止回阀","1250*630","个",1]
[475,"止回阀","800*400","个",1]
[476,"止回阀","800*630","个",1]
[477,"止回阀","500*320","个",1]
[478,"止回阀","500*500","个",1]
[479,"止回阀","1000*800","个",1]
[480,"止回阀","800*400","个",1]
[481,"止回阀","1250*630","个",1]
[482,"止回阀","800*400","个",1]
[483,"止回阀","800*500","个",1]
[484,"止回阀","1600*630","个",1]
[485,"止回阀","630*500","个",1]
[486,"止回阀","1250*500","个",1]
[487,"止回阀","1250*500","个",1]
[488,"止回阀","500*320","个",1]
[489,"止回阀","1000*1000","个",1]
[490,"止回阀","1000*1000","个",1]
[491,"止回阀","1600*800","个",1]
[492,"止回阀","1250*1000","个",1]
[493,"止回阀","1250*1000","个",1]
[494,"止回阀","1000*1000","个",1]
[495,"止回阀","1250*800","个",1]
[496,"轴流风机","43200m3/h 918pa 1450rpm 18.5kw ","个",1]
[497,"轴流风机","29520m3/h 378pa 1450rpm 5.5kw ","个",1]
[498,"阻抗复合型消声器","800*320","个",1,null,null,"长度1500"]
[499,"阻抗复合型消声器","1000*250","个",1,null,null,"长度1500"]
[500,"阻抗复合型消声器","1000*500","个",1,null,null,"长度1500"]
[501,"阻抗复合型消声器","800*630","个",1,null,null,"长度1500"]
[502,"阻抗复合型消声器","1000*630","个",1,null,null,"长度1500"]
[503,"阻抗复合型消声器","800*400","个",1,null,null,"长度1500"]
[504,"阻抗复合型消声器","1000*630","个",1,null,null,"长度1500"]
[505,"阻抗复合型消声器","1250*630","个",1,null,null,"长度1500"]
[506,"阻抗复合型消声器","1000*500","个",1,null,null,"长度1500"]
[507,"阻抗复合型消声器","1000*320","个",1,null,null,"长度1500"]
[508,"阻抗复合型消声器","1250*320","个",1,null,null,"长度1500"]
[509,"阻抗复合型消声器","800*630","个",2,null,null,"长度1000"]
[510,"阻抗复合型消声器","630*400","个",2,null,null,"长度1000"]
[511,"阻抗复合型消声器","500*500","个",1,null,null,"长度1000"]
[512,"阻抗复合型消声器","500*400","个",1,null,null,"长度1000"]
[513,"阻抗复合型消声器","500*400","个",1,null,null,"长度1000"]
[514,"阻抗复合型消声器","1250*630","个",2,null,null,"长度1500"]
[515,"阻抗复合型消声器","1000*630","个",1,null,null,"长度1500"]
[516,"阻抗复合型消声器","630*320","个",1,null,null,"长度1000"]
[517,"阻抗复合型消声器","400*250","个",1,null,null,"长度1000"]
[518,"阻抗复合型消声器","1250*630","个",1]
[519,"阻抗复合型消声器","500*320","个",2,null,null,"长度1000"]
[520,"阻抗复合型消声器","800*400","个",1,null,null,"长度1500"]
[521,"阻抗复合型消声器","1250*630","个",1,null,null,"长度1500"]
[522,"阻抗复合型消声器","1000*630","个",1,null,null,"长度1500"]
[523,"阻抗复合型消声器","800*630","个",1,null,null,"长度1000"]
[524,"阻抗复合型消声器","800*400","个",1,null,null,"长度1500"]
[525,"阻抗复合型消声器","1250*1600","个",1,null,null,"长度1500"]
[526,"阻抗复合型消声器","500*320","个",1,null,null,"长度1500"]
[527,"阻抗复合型消声器","1000*500","个",1,null,null,"长度1500"]
[528,"阻抗复合型消声器","800*500","个",1,null,null,"长度1500"]
[529,"阻抗复合型消声器","1250*630","个",1,null,null,"长度1500"]
[530,"阻抗复合型消声器","1600*630","个",1,null,null,"长度1500"]
[531,"阻抗复合型消声器","1250*500","个",1,null,null,"长度1500"]
[532,"阻抗复合型消声器","1250*500","个",1,null,null,"长度1500"]
[533,"阻抗复合型消声器","500*320","个",2,null,null,"长度1500"]
[534,"阻抗复合型消声器","1000*1000","个",1,null,null,"长度1500"]
[535,"阻抗复合型消声器","1250*500","个",1,null,null,"长度1500"]
[536,"阻抗复合型消声器","1000*1000","个",1,null,null,"长度1500"]
[537,"阻抗复合型消声器","1000*630","个",1,null,null,"长度1500"]
[538,"阻抗复合型消声器","1250*630","个",1,null,null,"长度1500"]
[539,"阻抗复合型消声器","1600*630","个",1,null,null,"长度1500"]
[540,"阻抗复合型消声器","1250*800","个",2,null,null,"长度1500"]
[541,"阻抗复合型消声器","2000*630","个",1,null,null,"长度1500"]
[542,"阻抗复合型消声器","1250*630","个",2,null,null,"长度1500"]
[543,"阻抗复合型消声器","1600*630","个",1,null,null,"长度1500"]
[544,"阻抗复合型消声器","500*400","个",1,null,null,"长度1000"]
[545,"阻抗复合型消声器","1600*630","个",1,null,null,"长度1500"]
[546,"阻抗复合型消声器","1250*630","个",1,null,null,"长度1500"]
[547,"阻抗复合型消声器","1250*800","个",1]
[null,"热源中心",null,"个"]
[1,"70°防火阀","800*630","个",1,null,null,"常开70°熔断关闭 "]
[2,"70°防火阀","800*630","个",1,null,null,"常开70°熔断关闭 "]
[3,"70°防火阀","250*200","个",1,null,null,"常开70°熔断关闭 "]
[4,"70°防火阀","200*120","个",1,null,null,"常开70°熔断关闭 "]
[5,"70°防火阀","800*630","个",1,null,null,"常开70°熔断关闭 "]
[6,"70°防火阀","800*630","个",1,null,null,"常开70°熔断关闭 "]
[7,"70°防火阀","630*500","个",1,null,null,"常开70°熔断关闭 "]
[8,"70°防火调节阀","200*120","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[9,"70°防火调节阀","320*200","个",1,null,null,"常开70°熔断关闭 带风量调节"]
[10,"单层百叶风口","1600*630","个",2,null,null,"叶片垂直 带调节阀"]
[11,"单层百叶风口","320*160","个",1]
[12,"单层百叶风口","1600*630","个",2,null,null,"叶片垂直 带调节阀"]
[13,"单层百叶风口","1250*500","个",2,null,null,"叶片垂直 带调节阀"]
[14,"单层百叶风口","320*160","个",3]
[15,"单层百叶风口","1600*630","个",2,null,null,"叶片垂直 带调节阀"]
[16,"单层百叶风口","1600*630","个",2,null,null,"叶片垂直 带调节阀"]
[17,"单层百叶风口","1250*500","个",2,null,null,"叶片垂直 带调节阀"]
[18,"防火风口","320*160","个",4,null,null,"常开70°熔断关闭 带风量调节"]
[19,"回风箱","1400*500*500","个",2]
[20,"可开百叶","1000*250","个",12,null,null,"带过滤网"]
[21,"可开百叶","700*250","个",45,null,null,"带过滤网"]
[22,"可开百叶","550*250","个",59,null,null,"带过滤网"]
[23,"可开铰链式百叶","1250*400","个",2,null,null,"带过滤网"]
[24,"可调条型风口","1000*137","个",24,null,null,"每台盘管两个"]
[25,"可调条型风口","800*137","个",90,null,null,"每台盘管两个"]
[26,"可调条型风口","600*171","个",24,null,null,"每台盘管一个"]
[27,"可调条型风口","500*137","个",70,null,null,"每台盘管两个"]
[28,"离心柜式风机箱","12810m3/h 368pa静319pa 550rpm 5.5kw 68db(A)","个",1,null,null,"防爆型"]
[29,"离心柜式风机箱","12810m3/h 368pa静319pa 550rpm 5.5kw 68db(A)","个",1,null,null,"防爆型"]
[30,"离心柜式风机箱","7420m3/h 409pa静370pa 700rpm 3kw 63db(A)","个",1]
[31,"离心柜式风机箱","12810m3/h 368pa静319pa 550rpm 5.5kw 68db(A)","个",1,null,null,"防爆型"]
[32,"离心柜式风机箱","12810m3/h 368pa静319pa 550rpm 5.5kw 68db(A)","个",1,null,null,"防爆型"]
[33,"离心柜式风机箱","7420m3/h 409pa静370pa 700rpm 3kw 63db(A)","个",1]
[34,"条型散流器","1000*171","个",6]
[35,"调节阀","200*120","个",2]
[36,"调节阀","320*250","个",4]
[37,"止回阀","800*630","个",1]
[38,"止回阀","800*630","个",1]
[39,"止回阀","630*500","个",1]
[40,"止回阀","1250*1000","个",1]
[41,"止回阀","1250*1000","个",1]
[42,"止回阀","630*500","个",1]
[43,"阻抗复合型消声器","800*630","个",1,null,null,"长度1500"]
[44,"阻抗复合型消声器","800*630","个",1,null,null,"长度1500"]
[45,"阻抗复合型消声器","630*500","个",1,null,null,"长度1500"]
[46,"阻抗复合型消声器","800*630","个",1,null,null,"长度1500"]
[47,"阻抗复合型消声器","1250*1000","个",1,null,null,"长度1500"]
[48,"阻抗复合型消声器","800*630","个",1,null,null,"长度1500"]
[49,"阻抗复合型消声器","1250*1000","个",1,null,null,"长度1500"]
[50,"阻抗复合型消声器","630*500","个",1,null,null,"长度1500"]
[null,"体育馆",null,"个"]
[1,"设备","离心式风机 EA(G)-1/2-5 860M3/H .25KW","个",1]
[2,"设备","离心式风机 EA(G)-1/2-1 1300M3/H  0.18KW","个",1]
[3,"设备","离心式风机 EA(G)-1/2-3 860M3/H 0.25KW","个",1]
[4,"设备","离心式风机 EA(G)-1/2-4 860M3/H  0.25 KW","个",1]
[5,"设备","离心式风机 EA(G)-1/2-2 3000M3/H 0.37KW","个",1]
[6,"设备","离心式风机 EA(G)-1/5-2 1780M3/H 0.18KW","个",1]
[7,"设备","离心式风机 560M3/H H=142Pa N=90W(220V)，噪声≤53dB(A) 管道式离心风机 ","个",1]
[8,"设备","离心式风机 EA(G)-1/4-3 1780M3/H 0.18KW","个",1]
[9,"设备","离心式风机 管道式离心风机 160M3/H H=122Pa N=25W(220V)，噪声≤45dB(A) ","个",1]
[10,"设备","离心式风机 EA(G)-1/4-2 1780M3/H 0.18M3/H","个",1]
[11,"设备","离心式风机 EA(G)-1/3-2 1780M3/H 0.18KW","个",1]
[12,"设备","离心式风机 EA(G)-2/1-3 5610M3/H 1.5 2F卫生间排风 2","个",1]
[13,"设备","离心式风机 EA(G)-2/1-4 5610M3/H 1.5 2F卫生间排风 2","个",1]
[14,"设备","离心式风机 EA(G)-1/5-4 860M3/H 250W舞美供电室事故排风 1","个",1]
[15,"设备","离心式风机 EA(G)-2/1-2 3500M3/H 2.2KW 6.0米标高右侧下方卫生间 2","个",1]
[16,"设备","离心式风机 EA(G)-2/1-1 3500M3/H 2.2KW落地安装6.0米标高右侧上方卫生间 2","个",1]
[17,"设备","离心式风机 EA/SE(G)-3-1 37860M3/H 13KW 59300M3/H 38KW 比赛大厅排风排烟 3","个",1]
[18,"设备","离心式风机 EA/SE(G)-3-2 37860M3/H 13KW 59300M3/H 38KW 比赛大厅排风排烟 3","个",1]
[19,"设备","离心式风机 EA/SE(G)-3-3 37860M3/H 13KW 59300M3/H 38KW 比赛大厅排风排烟 3","个",1]
[20,"设备","离心式风机 EA/SE(G)-3-4 37860/1359300/38比赛大厅排风排烟 3","个",1]
[21,"设备","离心式风机 EA/SE(G)-3-6 37860M3/H 13KW 59300M3/H 38KW 比赛大厅排风排烟 3","个",1]
[22,"设备","离心式风机 EA/SE(G)-3-7 37860M3/H 13KW 59300M3/H 38KW 比赛大厅排风排烟 3","个",1]
[23,"设备","离心式风机 EA/SE(G)-3-8 37860M3/H 13KW 59300M3/H 38KW 比赛大厅排风排烟 3","个",1]
[24,"设备","离心式风机 EA/SE(G)-3-9 37860/1359300/38比赛大厅排风排烟 3","个",1]
[25,"设备","离心式风机 EA/SE(G)-3-13 7860M3/H 13KW 59300M3/H 38KW 观众休息大厅排风排烟 3","个",1]
[26,"设备","离心式风机 EA/SE(G)-3-12 37860M3/H 13KW 59300M3/H 38KW 观众休息大厅排风排烟 3","个",1]
[27,"设备","离心式风机 EA/SE(G)-3-15 37860M3/H 13KW 59300M3/H 38KW 观众休息大厅排风排烟 3","个",1]
[28,"设备","轴流式风机 SE(G)-1/2-1 38800M3/H 18.5KW","个",1]
[29,"设备","轴流式风机 SE(G)-1/3-1 38800M3/H 18.5KW","个",1]
[30,"设备","轴流式风机 SE(G)-1/4-1    38800M3/H 18.5KW","个",1]
[31,"设备","轴流式风机 SE(G)-1/5-1 38800M3/H 18.5KW","个",1]
[32,"设备","轴流式风机 SE(G)-1/2-2 38800M3/H 18.5KW","个",1]
[33,"设备","轴流式风机 SP(G)-ST(05-11)-ME 15200M3/H 4KW","个",4]
[34,"设备","轴流式风机 SP(G)-ST(02-8)-1 62472M3/H 18.5KW 落地安装 2","个",1]
[35,"设备","轴流式风机 SP(G)-ST(02-2)-1-2 39204M3/H 11KW","个",1]
[36,"设备","轴流式风机 SP(G)-ST(02-2)-1-11 2200/3 2","个",1]
[37,"设备","轴流式风机 SP(G)-ST(05-5)-1 32400M3/H 7.5KW","个",1]
[38,"设备","轴流式风机 SP(G)-ST(02-1)-1-2 39204M3/H 11KW","个",1]
[39,"设备","轴流式风机 SP(G)-ST(02-7)-1 62472M3/H 18.5KW落地安装 2","个",1]
[40,"设备","轴流式风机 SP(G)-ST(02-1)-1-11 2200M3/H 3 KW","个",1]
[41,"设备","轴流式风机 SP(G)-ST(05-4)-1 32400M3/H 7.5KW","个",1]
[42,"设备","轴流式风机 SP(G)-ST(05-2)-ME15200M3/H 4 KW","个",1]
[43,"设备","轴流式风机 MA(G)-1/1-1 60000M3/H 18.5KW落地安装 1","个",1]
[44,"设备","轴流式风机 MA(G)-1/1-2 60000M3/H 18.5KW落地安装 1","个",1]
[45,"设备","轴流式风机 MA(G)-1/1-3 60000M3/H 18.5KW落地安装 1","个",1]
[46,"设备","轴流式风机 MA(G)-1/1-4 60000M3/H 18.5落地安装 1","个",1]
[47,"设备","轴流式风机 SE(G)-3-5 60096M3/H 30KW比赛大厅排烟 3","个",1]
[48,"设备","轴流式风机 SE(G)-3-1 3 23848M3/H 11KW层观众休息大厅排烟 3","个",1]
[49,"设备","轴流式风机 SE(G)-3-1 6 23848M3/H 11KW层观众休息大厅排烟 3","个",1]
[50,"设备","轴流式风机 SE(G)-3-10 60096M3/H 30KW比赛大厅排烟 3","个",1]
[51,"设备","轴流式风机 SE(G)-3-18 70100M3/H 30KW训练大厅排烟 3","个",1]
[52,"设备","轴流式风机 SE(G)-3-17 70100M3/H 30KW训练大厅排烟 3","个",1]
[53,"设备","轴流式风机 SP(G)-ST(02-10)-3 30780/7.5 2","个",1]
[54,"设备","轴流式风机 SP(G)-ST(02-5)-3 30780/7.5 2","个",1]
[55,"设备","轴流式风机 SE(G)-4-1 70100M3/H 30KW落地安装观众休息大厅排烟 4","个",1]
[56,"设备","轴流式风机 SE(G)-4-3 36015M3/H 18.5KW落地安装B1-2F贵宾小房间排烟 4","个",1]
[57,"设备","轴流式风机 SE(G)-4-2 70100M3/H 30KW落地安装观众休息大厅排烟 4","个",1]
[58,"设备","换气扇 天花板管道式换气扇 风量：150m3/h 风压：180Pa 150","个",3]
[59,"风阀","FD 630*250  ","个",1]
[60,"风阀","FD 500*400  ","个",8]
[61,"风阀","FD 1000*400 ","个",8]
[62,"风阀","FD 1600*450  ","个",1]
[63,"风阀","FD 1000*450  ","个",4]
[64,"风阀","FD 800*400  ","个",4]
[65,"风阀","FD 1250*400  ","个",3]
[66,"风阀","FD 2000*2000","个",4]
[67,"风阀","止回阀 D910","个",3]
[68,"风阀","止回阀 D860","个",2]
[69,"风阀","止回阀 250*250  ","个",1]
[70,"风阀","止回阀 400*250  ","个",1]
[71,"风阀","止回阀 500*250 ","个",1]
[72,"风阀","止回阀 320*250  ","个",1]
[73,"风阀","止回阀 400*400  ","个",1]
[74,"风阀","止回阀 D610  ","个",5]
[75,"风阀","止回阀 D1100  ","个",1]
[76,"风阀","止回阀 900*400  ","个",1]
[77,"风阀","止回阀 800*800  ","个",1]
[78,"风阀","止回阀 2500*550  ","个",1]
[79,"风阀","止回阀 1600*630  ","个",1]
[80,"风阀","止回阀 800*400   ","个",1]
[81,"风阀","止回阀 D1060  ","个",4]
[82,"风阀","止回阀 1600*800  ","个",1]
[83,"风阀","止回阀 1250*1250  ","个",2]
[84,"风阀","止回阀 800*1250   ","个",2]
[85,"风阀","止回阀 630*630  ","个",2]
[86,"风阀","止回阀 1400*1400 ","个",11]
[87,"风阀","止回阀 D1110  ","个",2]
[88,"风阀","止回阀 D660  ","个",2]
[89,"风阀","止回阀 D1210   ","个",4]
[90,"风阀","止回阀 D760 ","个",2]
[91,"风阀","止回阀 D810  ","个",1]
[92,"风阀","对开多叶调节阀 1250*600  ","个",2]
[93,"风阀","对开多叶调节阀 1000*700  ","个",2]
[94,"风阀","对开多叶调节阀 400*400  ","个",7]
[95,"风阀","对开多叶调节阀 630*630  ","个",4]
[96,"风阀","对开多叶调节阀 630*500  ","个",3]
[97,"风阀","对开多叶调节阀 600*200  ","个",13]
[98,"风阀","对开多叶调节阀 400*320  ","个",10]
[99,"风阀","对开多叶调节阀 320*250  ","个",6]
[100,"风阀","对开多叶调节阀 250*200 ","个",1]
[101,"风阀","对开多叶调节阀 500*320 ","个",18]
[102,"风阀","对开多叶调节阀 500*400  ","个",4]
[103,"风阀","对开多叶调节阀 500*200  ","个",6]
[104,"风阀","对开多叶调节阀 250*250  ","个",12]
[105,"风阀","对开多叶调节阀 320*320  ","个",2]
[106,"风阀","对开多叶调节阀 200*200  ","个",1]
[107,"风阀","对开多叶调节阀 200*120  ","个",4]
[108,"风阀","对开多叶调节阀 320*200  ","个",12]
[109,"风阀","对开多叶调节阀 1400*630  ","个",4]
[110,"风阀","对开多叶调节阀 2000*800  ","个",4]
[111,"风阀","对开多叶调节阀 630*450  ","个",4]
[112,"风阀","对开多叶调节阀 800*500  ","个",4]
[113,"风阀","对开多叶调节阀 1000*550  ","个",2]
[114,"风阀","对开多叶调节阀 630*320 ","个",6]
[115,"风阀","对开多叶调节阀 500*500 ","个",2]
[116,"风阀","对开多叶调节阀 D1676","个",6]
[117,"风阀","对开多叶调节阀 D1168 ","个",18]
[118,"风阀","对开多叶调节阀 D914 ","个",20]
[119,"风阀","对开多叶调节阀 D660 ","个",18]
[120,"风阀","对开多叶调节阀 D533 ","个",2]
[121,"风阀","对开多叶调节阀 D305 ","个",{"v":9.2,"d":"9"}]
[122,"风阀","对开多叶调节阀 250*200","个",5]
[123,"风阀","对开多叶调节阀 800*320","个",20]
[124,"风阀","调节阀 250*160 ","个",40]
[125,"风阀","调节阀 320*200","个",1]
[126,"风阀","调节阀 200*200 ","个",5]
[127,"风阀","调节阀 250*200 ","个",10]
[128,"风阀","调节阀 250*120 ","个",10]
[129,"风阀","调节阀 250*250 ","个",15]
[130,"风阀","调节阀 320*160 ","个",18]
[131,"风阀","调节阀 320*320 ","个",1]
[132,"风阀","调节阀 500*320 ","个",1]
[133,"风阀","调节阀 200*160 ","个",23]
[134,"风阀","调节阀 400*320 ","个",2]
[135,"风阀","调节阀 400*200 ","个",1]
[136,"风阀","调节阀 500*200 ","个",3]
[137,"风阀","调节阀 600*200 ","个",13]
[138,"风阀","调节阀 320*250 ","个",7]
[139,"风阀","调节阀 2000*800 ","个",2]
[140,"风阀","电动对开多叶调节阀 400*400 ","个",7]
[141,"风阀","电动对开多叶调节阀 630*630 ","个",4]
[142,"风阀","电动对开多叶调节阀 630*500 ","个",2]
[143,"风阀","电动对开多叶调节阀 1250*800 ","个",2]
[144,"风阀","电动对开多叶调节阀 1600*800 ","个",1]
[145,"风阀","电动对开多叶调节阀 1500*800 ","个",2]
[146,"风阀","电动对开多叶调节阀 1250*1000 ","个",1]
[147,"风阀","电动对开多叶调节阀 630*450 ","个",2]
[148,"风阀","电动对开多叶调节阀 1250*500 ","个",2]
[149,"风阀","电动对开多叶调节阀 500*500 ","个",4]
[150,"风阀","电动对开多叶调节阀 D660","个",10]
[151,"风阀","电动对开多叶调节阀 D1676 ","个",2]
[152,"风阀"," FDH D910","个",3]
[153,"风阀","FDH 800*400","个",32]
[154,"风阀"," FDH 1100*500","个",3]
[155,"风阀"," FDH 800*320","个",1]
[156,"风阀"," FDH 630*250","个",1]
[157,"风阀"," FDH 1400*400","个",7]
[158,"风阀"," FDH 630*400","个",1]
[159,"风阀"," FDH 300*600","个",2]
[160,"风阀"," FDH 1000*320","个",1]
[161,"风阀"," FDH 900*630","个",2]
[162,"风阀"," FDH 630*800 ","个",1]
[163,"风阀"," FDH 900*650 ","个",1]
[164,"风阀","FDH 1400*800 ","个",10]
[165,"风阀"," FDH 1250*800 ","个",26]
[166,"风阀"," FDH D1210 ","个",2]
[167,"风阀"," FDH D810 ","个",1]
[168,"风阀"," FDH 2000*800 ","个",1]
[169,"风阀"," FDEH 1400*400","个",4]
[170,"风阀"," FDEH 1100*500","个",2]
[171,"风阀","FDEH 630*400 ","个",4]
[172,"风阀"," FDEH 2000*800 ","个",12]
[173,"风阀"," FDEH 1600*800 ","个",1]
[174,"风阀"," FDEH 500*800 ","个",1]
[175,"风阀"," FDEH 1250*800 ","个",1]
[176,"风阀"," FDEH 900*630 ","个",1]
[177,"风阀"," FDEH 800*500 ","个",1]
[178,"风阀"," BECH 800*400","个",32]
[179,"风阀"," BECH 800*320","个",1]
[180,"风阀"," BECH 630*250","个",1]
[181,"风阀"," BECH 300*600","个",2]
[182,"风阀"," BECH 1000*320","个",1]
[183,"风阀"," BECH 630*400 ","个",5]
[184,"风阀"," BECH 250*500 ","个",1]
[185,"风阀"," BECH 1400*800 ","个",8]
[186,"风阀"," BECH 1250*800 ","个",23]
[187,"风阀"," FD 250*250 ","个",12]
[188,"风阀"," FD 320*250 ","个",11]
[189,"风阀"," FD 400*250 ","个",3]
[190,"风阀"," FD 500*250 ","个",4]
[191,"风阀"," FD 400*400 ","个",6]
[192,"风阀","FD 320*200 ","个",3]
[193,"风阀"," FD 800*250","个",3]
[194,"风阀","FD 200*200 ","个",3]
[195,"风阀"," FD 400*500 ","个",2]
[196,"风阀"," FD 250*160 ","个",1]
[197,"风阀"," FD 400*320 ","个",{"v":5.1,"d":"5"}]
[198,"风阀","FD 630*400 ","个",3]
[199,"风阀"," FD 250*200 ","个",4]
[200,"风阀"," FD 400*200 ","个",1]
[201,"风阀"," FD 1600*800 ","个",10]
[202,"风阀"," FD 1600*1250 ","个",1]
[203,"风阀"," FD 1250*800 ","个",8]
[204,"风阀"," FD 1250*1000 ","个",1]
[205,"风阀"," FD 1200*2000 ","个",6]
[206,"风阀"," FD 1000*2000 ","个",2]
[207,"风阀"," FD 900*400 ","个",2]
[208,"风阀"," FD 1000*800 ","个",2]
[209,"风阀"," FD 630*320 ","个",4]
[210,"风阀"," FD 200*250 ","个",1]
[211,"风阀"," FD 320*320 ","个",1]
[212,"风阀"," FD 1500*2000 ","个",2]
[213,"风阀","FD 1100*630 ","个",2]
[214,"风阀"," FD 1250*1250","个",4]
[215,"风阀","FD 2400*550 ","个",2]
[216,"风阀"," FD 2200*500 ","个",2]
[217,"风阀"," FD 630*630 ","个",2]
[218,"风阀"," FD 200*320 ","个",1]
[219,"风阀"," FD 500*500 ","个",4]
[220,"风阀"," FD 630*800 ","个",2]
[221,"风阀"," BEC 400*320 ","个",1]
[222,"风阀"," FVD 320*160 ","个",1]
[223,"风阀"," FVD 500*250 ","个",3]
[224,"风阀"," FVD 400*160 ","个",1]
[225,"风阀","FVD 630*400","个",1]
[226,"风阀","FVD 800*200 ","个",1]
[227,"风阀"," FVD 200*160 ","个",1]
[228,"风阀"," FVD 400*200","个",1]
[229,"风阀"," FVD 500*200 ","个",1]
[230,"风阀"," FVD 250*160 ","个",2]
[231,"风阀"," FVD 250*200 ","个",2]
[232,"风阀","FD 900*400","个",5]
[233,"风阀","FD 1400*400 ","个",1]
[234,"风阀","FD 2000*800 ","个",7]
[235,"风阀","FD 800*800 ","个",1]
[236,"风阀","FD 1000*630 ","个",1]
[237,"风阀","FD 1500*800 ","个",2]
[238,"风阀","FD 2400*630 ","个",2]
[239,"风阀","FD 450*400 ","个",2]
[240,"风阀","FD D100 ","个",2]
[241,"风阀","FDH 1400*1400 ","个",11]
[242,"风阀","FDH 800*2000 ","个",10]
[243,"风阀","FDH D1110 ","个",2]
[244,"风阀","FDH 1400*800 ","个",1]
[245,"风阀","FDH D660 ","个",2]
[246,"风阀","FDH 500*800 ","个",2]
[247,"风阀","FDH D1210 ","个",2]
[248,"风阀","FDS 800*400 ","个",4]
[249,"风阀","FDS 1600*630 ","个",2]
[250,"风阀","FDS 2400*400 ","个",2]
[251,"风阀","FDS 630*630 ","个",2]
[252,"风阀","FDS 900*800 ","个",4]
[253,"风阀","FDS 1250*500 ","个",1]
[254,"风阀","FDS 1500*500 ","个",1]
[255,"风阀","FDS 2000*100 ","个",1]
[256,"风阀","D613","个",2]
[257,"风阀","FDS 2000*800 ","个",4]
[258,"风阀","FDS 2500*550 ","个",1]
[259,"风阀","FDS 2000*1000 ","个",1]
[260,"风阀","FDS D1060 ","个",4]
[261,"风阀","FDS 1250*800 ","个",8]
[262,"风阀","FDS D760 ","个",2]
[263,"风阀","FDS 1000*500 ","个",4]
[264,"风阀"," BECS 1250*800 ","个",4]
[265,"风阀","MEE 2200*450 ","个",2]
[266,"风阀"," MEES 2000*800 ","个",9]
[267,"风阀"," MEES 1250*800 ","个",3]
[268,"风阀","FD 1600*630","个",2]
[269,"风阀","FD 1000*800","个",6]
[270,"风阀","FD 1250*630","个",2]
[271,"风口","百叶风口 320*320","个",1]
[272,"风口","百叶风口 320*250 ","个",1]
[273,"风口","百叶风口 1250*600 ","个",2]
[274,"风口","百叶风口 1000*700 ","个",2]
[275,"风口","AV 600*900","个",28]
[276,"风口","AV 500*500","个",1]
[277,"风口","AV 600*600","个",2]
[278,"风口","AV 550*400","个",1]
[279,"风口","AV 300*600","个",1]
[280,"风口","AV 300*600 ","个",5]
[281,"风口","AV 600*600 ","个",1]
[282,"风口","AV 550*400 ","个",1]
[283,"风口","AV 700*1200 ","个",3]
[284,"风口","AV 1500*2000 ","个",1]
[285,"风口","AV 800*800 ","个",12]
[286,"风口"," AV 600*900 ","个",7]
[287,"风口"," AV 2000*3500 ","个",1]
[288,"风口"," AV 700*1200 ","个",2]
[289,"风口"," AV 1500*500 ","个",1]
[290,"风口"," AV 2000*800 ","个",2]
[291,"风口"," AV 1200*2000 ","个",2]
[292,"风口"," AV 1000*2000 ","个",2]
[293,"风口"," AV 150*150 ","个",20]
[294,"风口"," AV 1500*2000 ","个",1]
[295,"风口"," AV/D 150*150 ","个",67]
[296,"风口"," AV/D 500*250 ","个",1]
[297,"风口"," AV/D 200*200 ","个",9]
[298,"风口"," AV/D 320*250 ","个",4]
[299,"风口"," AV/D 250*400 ","个",1]
[300,"风口"," AV/D 160*160 ","个",8]
[301,"风口"," AV/D 320*320 ","个",8]
[302,"风口"," AV/D 500*1000 ","个",1]
[303,"风口"," AV/D 400*630 ","个",1]
[304,"风口"," AV/D 200*150 ","个",4]
[305,"风口"," AV/D 200X150 ","个",9]
[306,"风口"," AV/D 150*100 ","个",2]
[307,"风口"," AV/D 1200*1200 ","个",20]
[308,"风口"," AV/D 900*900 ","个",36]
[309,"风口"," AV/D 600*900 ","个",4]
[310,"风口"," AV/D 1000*1000 ","个",16]
[311,"风口"," AV/D 1800*1200 ","个",8]
[312,"风口"," AV/D 1100*1100 ","个",2]
[313,"风口","AV/D 1000*1100 ","个",2]
[314,"风口"," AV 800*250 ","个",4]
[315,"风口"," AV 160*160 ","个",1]
[316,"风口"," AV 120*120 ","个",1]
[317,"风口"," AV 250*200 ","个",3]
[318,"风口"," AV 1200*2000 ","个",4]
[319,"风口","AV 150*150 ","个",3]
[320,"风口","AV 500*500 ","个",3]
[321,"风口","GF 3000*2400","个",2]
[322,"风口","GF 2000*2000 ","个",7]
[323,"风口","GF 2000*200 ","个",1]
[324,"风口","GF 3000*2400 ","个",2]
[325,"风口","GF 10000*2000 ","个",2]
[326,"风口","GF 2100*2000 ","个",2]
[327,"风口","GF 1400*2000 ","个",1]
[328,"风口","GF 1000*2000 ","个",1]
[329,"风口","GF 2400*630 ","个",1]
[330,"风口","百叶风口（新风口） 200*200 ","个",28]
[331,"风口","百叶风口（新风口） 300*300 ","个",26]
[332,"风口","百叶风口（新风口） 250*250 ","个",7]
[333,"风口","百叶风口（新风口） 150*150 ","个",12]
[334,"风口","百叶风口（新风口） 200*200","个",15]
[335,"风口","百叶风口（新风口） 150*150","个",13]
[336,"风口","百叶风口（新风口）800*800","个",3]
[337,"风口","百叶风口（新风口） 300*300","个",9]
[338,"风口","防火风口GFS 850*700 ","个",2]
[339,"风口","防火风口GFS 1500*1000 ","个",1]
[340,"风口","正压送风口 1250*630 ","个",2]
[341,"风口","正压送风口 1000*700 ","个",2]
[342,"风口","单层百叶风口E2 1000*69 ","个",48]
[343,"风口","BH 600*200 ","个",26]
[344,"风口","BH 500*200 ","个",6]
[345,"风口","BV/D 400*200 ","个",25]
[346,"风口","BV/D 900*900 ","个",12]
[347,"风口","百叶风口K 1000*600 ","个",3]
[348,"风口","百叶风口K 1200*1000 ","个",6]
[349,"风口","百叶风口K 1000*800 ","个",3]
[350,"风口","百叶风口K D100 ","个",1]
[351,"风口","百叶风口K 2000*2000","个",4]
[352,"风口","百叶风口K 500*250","个",64]
[353,"风口","百叶风口K 1000*250","个",48]
[354,"风口","百叶风口K 800*250","个",86]
[355,"风口","单层百叶风口E4 1000*137 ","个",34]
[356,"风口","ZA/D 2000*800 ","个",4]
[357,"风口","电动风口VS D400 ","个",66]
[358,"风口","防虫风口 630*630","个",2]
[359,"风口","防虫风口 250*250","个",1]
[360,"风口","防虫风口 500*500","个",2]
[361,"风口","防虫风口 D100 ","个",2]
[362,"风口","AV/D 200*200 ","个",14]
[363,"风口","AD D440","个",140]
[364,"风口","百叶风口 2500*1000","个",2]
[365,"风口","送风口E4 1000*137","个",8]
[366,"风口","送风口BV 250*200","个",4]
[367,"风口","防虫百叶风口 500*550","个",1]
[368,"风口","TCD D1213","个",369]
[369,"风口","STD D134","个",2912]
[370,"消声器","ZKA1.5 1600×800","个",2]
[371,"消声器","ZKA1.5 1600*1250 ","个",1]
[372,"消声器","ZKA1.5 1250×800 ","个",1]
[373,"消声器","ZKA1.5 1400*630 ","个",2]
[374,"消声器","ZKA1.5 1600*630 ","个",2]
[375,"消声器","ZKB1.0 1000*400 ","个",1]
[376,"消声器","ZKB1.0 630*630","个",2]
[377,"消声器","ZKB1.0 630*400 ","个",1]
[378,"消声器","ZKB1.5 1400*1400 ","个",11]
[379,"消声器","ZKB1.5 2000*800 ","个",21]
[380,"消声器","ZKB1.5 1250*800","个",2]
[381,"消声器","ZKB1.5 1600*630 ","个",2]
[382,"静压箱","1900*1100*800","个",1]
[383,"静压箱","1600*1800*2400","个",1]
[384,"静压箱","1900*1100*800","个",1]
[385,"静压箱","1600*800*2400","个",1]
[386,"静压箱","2500*900*1000","个",1]
[387,"静压箱","3000*2100*1200H","个",1]
[388,"静压箱","3400*1800*900","个",1]
[389,"静压箱","3300*2400*1000","个",2]
[390,"静压箱","3400*1800*900","个",1]
[391,"静压箱","3600*1400*600","个",1]
[392,"静压箱","3600*1400*600","个",1]
[393,"静压箱","3600*1400*600","个",1]
[394,"静压箱","2600*1700*800","个",1]
[395,"静压箱","2700*2000*1200","个",2]
[396,"静压箱","2700*800*1200","个",2]
[397,"风机","减震器","个",126]
[398,"静压箱","送风静压箱1200x250x250","个","10"]
[399,"风口","可开百叶（带滤网）回风口550x250","个","47"]
[400,"风口","可开百叶（带滤网）回风口600x250","个","1"]
[401,"风口","可开百叶（带滤网）回风口700x250","个","1"]
[402,"风口","可开百叶（带滤网）回风口1000X250","个","1"]
[403,"风口","送风百叶风口 1000x137","个","47"]
[404,"风口","送风百叶风口 900x171","个","28"]
[405,"风口","送风百叶风口1000x171","个","36"]
[406,"设备","离心式风机 3470M3/H 1.1 KWEA(G)-B1/1-1","个",1]
[407,"设备","离心式风机 2250M3/H 1.1KW EA(G)-B1/4-1","个",1]
[408,"设备","离心式风机 4280M3/H 1.1KW EA(G)-B1/5-3","个",1]
[409,"设备","离心式风机 3060M3/H 1.1KW SA(G)-B1/5-3","个",1]
[410,"设备","离心式风机 25600M3/H 8.5KW 37700/24 KW EA/SE(G)-B1/2-1","个",1]
[411,"设备","离心式风机 25600M3/H 8.5KW 37700/24 KW EA/SE(G)-B1/3-1","个",1]
[412,"设备","离心式风机 25600M3/H 8.5KW 37700/24 KW EA/SE(G)-B1/2-2","个",1]
[413,"设备","离心式风机 25600M3/H 8.5KW 37700/24 KW EA/SE(G)-B1/3-2","个",1]
[414,"设备","离心式风机 25600M3/H 8.5KW 37700/24 KW EA/SE(G)-B1/5-1","个",1]
[415,"设备","离心式风机 25600M3/H 8.5KW 37700M3/H 24 KW EA/SE(G)-B1/5-2","个",1]
[416,"设备","离心式风机25600M3/H 8.5KW 37700M3/H 24 KWEA/SE(G)-B1/6-2","个",1]
[417,"设备","离心式风机 25600M3/H 8.5KW 37700M3/H 24 KWEA/SE(G)-B1/6-1","个",1]
[418,"设备","离心式风机 23300M3/7.5 KW SA/MA(G)-B1/5-2","个",1]
[419,"设备","离心式风机 23300M3/7.5 KW SA/MA(G)-B1/5-1","个",1]
[420,"设备","离心式风机 9120M3/2.8 KW 15000/8 KWSA/MA(G)-B1/5-5","个",1]
[421,"设备","离心式风机 3060M3/1.1 KWEA(G)-B1/5-4","个",1]
[422,"设备","轴流式风机 17100M3/5.5KW SP(G)-ST(02-4)-B1-1","个",1]
[423,"设备","轴流式风机 27500M3/7.5KW SP(N)-ST2-B1-1","个",1]
[424,"设备","离心式风机箱 25600M3 8.5KW 37700M3/24 KWEA/SE(G)-B1/1-1","个",1]
[425,"设备","离心式风机箱 25600M3/8.5KW 37700M3/24KW EA/SE(G)-B1/1-2","个",1]
[426,"消声","消声器1.0M 500*400","个",5]
[427,"消声","消声器1.0M 630*320","个",1]
[428,"消声","消声器1.5M 1250*1000","个",13]
[429,"消声","消声器1.5M 2000*500","个",9]
[430,"消声","消声器1.5M 1000*1000","个",2]
[431,"消声","消声器1.5M 1600*630","个",2]
[432,"风阀","止回阀 500*400","个",3]
[433,"风阀","止回阀 630*320","个",1]
[434,"风阀","止回阀 1000*1250","个",2]
[435,"风阀","止回阀 1250*1000","个",8]
[436,"风阀","止回阀 1000*1000","个",2]
[437,"风阀","对开多叶调节阀 1250*400","个",9]
[438,"风阀","对开多叶调节阀 1600*400","个",3]
[439,"风阀","对开多叶调节阀 1000*320","个",9]
[440,"风阀","对开多叶调节阀 1000*400","个",3]
[441,"风阀","对开多叶调节阀 2000*500","个",1]
[442,"风阀","对开多叶调节阀 1000*500","个",1]
[443,"风阀","对开多叶调节阀 500*500","个",2]
[444,"风阀","FDH 1000*1250","个",2]
[445,"风阀","FDH 2000*500","个",1]
[446,"风阀","FDH 1000*1000","个",4]
[447,"风阀","FDH 1250*1000","个",8]
[448,"风阀","FDH 1250*630","个",2]
[449,"风阀","FDH 1600*630","个",1]
[450,"风阀","FDEH 2000*500","个",8]
[451,"风阀","FDEH 1000*1000","个",2]
[452,"风阀","FDS 1000*1000","个",2]
[453,"风阀","FDS 1000*500","个",3]
[454,"风阀","FDS 500*500","个",2]
[455,"风阀","FDS 630*800","个",1]
[456,"风阀","FDS 1250*1000","个",3]
[457,"风阀","FDS 2000*500","个",1]
[458,"风口","AV 400*400","个",8]
[459,"风口","AV 400*320","个",2]
[460,"风口","AV 800*250","个",16]
[461,"风口","AV 1500*1100","个",1]
[462,"风口","AV 1600*1800","个",3]
[463,"风口","网式风口R 500*400","个",4]
[464,"风口","网式风口R 1250*1000","个",7]
[465,"风口","网式风口R 2000*500","个",1]
[466,"风口","网式风口R 1000*1000","个",6]
[467,"风口","网式风口R 1250*630","个",2]
[468,"风口","网式风口R 1600*630","个",1]
[469,"风口","AV/D 800*250","个",136]
[470,"风口","BV/D 1400*2300","个",1]
[471,"风口","BV/D 1250*1000","个",2]
[null,"体育场"]
[1,"风机","离心式风机 5000/3.0 EA(S)-1/3-3","台",1]
[2,"风机","离心式风机 9500/3.0 EA(S)-1/2-1","台",1]
[3,"风机","离心式风机 2250/1.1 EA(S)-1/4-1","台",1]
[4,"风机","离心式风机 800/0.09 EA(S)-1/2-2","台",1]
[5,"风机","离心式风机 2250/1.5 EA(S)-1/4-2","台",1]
[6,"风机","离心式风机 2520/0.75 EA(S)-1/4-4","台",1]
[7,"风机","离心式风机 2520/0.75 EA(S)-1/4-3","台",1]
[8,"风机","离心式风机 1678/0.45EA(S)-1/1-1","台",1]
[9,"风机","离心式风机 2520/0.75 EA(S)-1/4-5","台",1]
[10,"风机","离心式风机 2250/1.1 EA(S)-1/1-2","台",1]
[11,"风机","离心式风机 1200/0.25EA(S)-1/1-3","台",1]
[12,"风机","离心式风机 1200/0.25 EA(S)-1/2-3","台",1]
[13,"风机","离心式风机 1678/0.45 EA(S)-1/5-2","台",1]
[14,"风机","离心式风机 离心管道风机（防爆型） 560CMH，H=142Pa， N=90W(220V)，噪声<55dB(A)","台",1]
[15,"风机","离心式风机 1000/0.25 EA(S)-1/5-3","台",1]
[16,"风机","离心式风机 9100/4 EA(S)1/-5-1","台",1]
[17,"风机","离心式风机 18000M3/H EA(S)-2/6-1","台",3]
[18,"风机","离心式风机 2250/1.1 EA(S)-1/3-5","台",1]
[19,"风机","离心式风机18000M3/H EA(S)-1/2/6-2","台",2]
[20,"风机","离心式风机 F5 2000M3/H","台",2]
[21,"风机","离心式风机 F4 3000M3/H","台",2]
[22,"风机","离心式风机 F6 1200M3/H","台",3]
[23,"风机","离心式风机 EA(S)-2/6-2 18000/7.5","台",1]
[24,"风机","离心式风机 EA(S)-2/6-1 18000/7.5","台",1]
[25,"风机","离心式风机 F3 280M3/H","台",1]
[26,"风机","离心式风机 EA(S)-4/9-28100/3","台",1]
[27,"风机","离心式风机 EA(S)-4/9-18100/3","台",1]
[28,"风机","轴流式风机 63090/30SE(S)-1/3-1","台",1]
[29,"风机","轴流式风机 63090/30SE(S)-1/4-2","台",1]
[30,"风机","轴流式风机 63090/30SE(S)-1/3-2","台",1]
[31,"风机","轴流式风机 27238/11SE(S)-1/2-1","台",1]
[32,"风机","轴流式风机 34047/15.0SE(S)-1/2-2","台",1]
[33,"风机","轴流式风机 27238/11SE(S)-1/1-1","台",1]
[34,"风机","轴流式风机 24514/11SE(S)-1/1-2","台",1]
[35,"风机","轴流式风机 63090/30SE(S)-1/4-1","台",1]
[36,"风机","轴流式风机 63090/30SE(S)-1/5-2","台",1]
[37,"风机","轴流式风机 63090/30SE(S)-1/5-1","台",1]
[38,"风机","轴流式风机 F1 1300M3/H","台",15]
[39,"风机","轴流式风机 F2  350M3/H","台",20]
[40,"风机","轴流式风机 SE(S)-3/8-116090/5.5","台",1]
[41,"风机","轴流式风机 SE(S)-3/8-216090/5.5","台",1]
[42,"风机","轴流式风机 F7 900M3/H","台",1]
[43,"风口","BH/D 630×400","个",2]
[44,"风机"," 2520/0.75 EA(S)-1/3-4","台",1]
[45,"风口","BH/D 500*250","台",1]
[46,"风机"," 3210/1.5 EA(S)-1/3-1","台",1]
[47,"风口","BH/D 500×320","个",1]
[48,"风机"," 2520/0.75 EA(S)-1/3-2","台",1]
[49,"消声器","ZKB1.0 630×400","个",3]
[50,"消声器","ZKB1.0 500×250","个",2]
[51,"消声器","ZKB1.0 400×320","个",3]
[52,"消声器","ZKB1.0 500×320","个",1]
[53,"消声器","ZKB1.0 800×400","个",1]
[54,"消声器","ZKB1.0 1000×400","个",3]
[55,"消声器","ZKB1.0 400×250","个",2]
[56,"消声器","ZKB1.0 800*500","个",1]
[57,"消声器","ZKB1.0 630×630","个",2]
[58,"消声器","ZKB1.0 800×500","个",7]
[59,"消声器","ZKB1.0 1000×500","个",2]
[60,"消声器","ZKB1.0 630*400","个",2]
[61,"消声器","ZKB1.0 630X250","个",2]
[62,"消声器","ZKB1.5 1250×400","个",1]
[63,"消声器","ZKB1.5 1000×500","个",5]
[64,"消声器","ZP1.0 400X320","个",1]
[65,"消声器","ZP1.0 500*400","台",2]
[66,"消声器","ZP1.0 630X1200","个",2]
[67,"消声器","ZP1.5 1000X630","个",2]
[68,"消声器","ZP1.5 800X630","个",2]
[69,"消声器","ZP1.5 1000X400","个",2]
[70,"风口","BH/D 500×250","个",4]
[71,"风口","BH/D 500*300","个",8]
[72,"风口","BH/D 200*150","个",14]
[73,"风口","BH/D 150*150","个",10]
[74,"风口","BH/D 600*300","个",4]
[75,"风口","BH/D 320×200","个",2]
[76,"风口","BH/D 200*200","个",21]
[77,"风口","BH/D 600*250","个",4]
[78,"风口","BH/D 400×250","个",4]
[79,"风口","BH/D 150*100","个",10]
[80,"风口","BH/D 250×120","个",8]
[81,"风口","BH/D 200X120","个",14]
[82,"风口","防虫百叶风口 630X400","个",4]
[83,"风口","防虫百叶风口 500×630","个",1]
[84,"风口","防虫百叶风口 320×200","个",1]
[85,"风口","防虫百叶风口 400×250","个",2]
[86,"风口","防虫百叶风口 400×200","个",1]
[87,"风口","防虫百叶风口 320×120","个",2]
[88,"风口","防虫百叶风口 800×400","个",3]
[89,"风口","防虫百叶风口 630×500","个",1]
[90,"风口","防虫百叶风口 1250×800","个",3]
[91,"风口","防虫百叶风口 800×500","个",4]
[92,"风口","防虫百叶风口 800×550","个",2]
[93,"风口","防虫百叶风口 1600×630","个",2]
[94,"风口","防虫百叶风口 630×630","个",2]
[95,"风口","防虫百叶风口 1000×400","个",1]
[96,"风口","防虫百叶风口 1250×400","个",1]
[97,"风口","防虫百叶风口 1000×500","个",3]
[98,"风口","防虫百叶风口 320×160","个",4]
[99,"风口","防虫百叶风口 320*320","个",26]
[100,"风口","防虫百叶风口 200*200","个",18]
[101,"风口","防虫百叶风口 400×320","个",2]
[102,"风口","防虫百叶风口 500×400","个",2]
[103,"风口","防虫百叶风口 320×250","个",3]
[104,"风口","防虫百叶风口 630X250","个",2]
[105,"风口","防虫百叶风口 800X630","个",2]
[106,"风口","防虫百叶风口 250×120","个",2]
[107,"风口","防虫百叶风口 200*320","个",1]
[108,"风口","BH 250*150","个",16]
[109,"风口","BH 200*150","个",32]
[110,"风口","BH 400×200","个",4]
[111,"风口","BH 150*100","个",28]
[112,"风口","BH 150*150","个",47]
[113,"风口","BH 250×120","个",4]
[114,"风口","BH 320×200","个",10]
[115,"风口","BH 200*200","个",16]
[116,"风口","BH 200*400","个",1]
[117,"风口","BH 300*150","个",4]
[118,"风口","BH 600*400","个",9]
[119,"风口","BH 1400×800","个",16]
[120,"风口","BH 1200*700","个",1]
[121,"风口","BH 1000×400","个",3]
[122,"风口","BH 900*600","个",1]
[123,"风口","BH 800*600","个",3]
[124,"风口","BH 900*400","个",1]
[125,"风口","BH 800×400","个",9]
[126,"风口","BH 800×500","个",5]
[127,"风口","BH 600*300","个",1]
[128,"风口","BH 700*400","个",1]
[129,"风口","BH 1200*800","个",4]
[130,"风口","BH 1400*800","个",8]
[131,"风口","BH 100*100","个",3]
[132,"风口","BH 630×500","个",1]
[133,"风口","BH 500*300","个",2]
[134,"风口","AV/D 160×160","个",110]
[135,"风口","AV/D 200*200","个",98]
[136,"风口","AV/D 120×120","个",6]
[137,"风口","AV/D 200X120","个",7]
[138,"风口","AH 200*200","个",18]
[139,"风口","AV 200X120","个",10]
[140,"风口","AV 200*200","个",4]
[141,"风口","AV 250×120","个",2]
[142,"风阀","止回阀 400×320","个",1]
[143,"风阀","止回阀 320×200","个",3]
[144,"风阀","止回阀 320×250","个",2]
[145,"风阀","止回阀 250*160","个",1]
[146,"风阀","止回阀 800×630","个",1]
[147,"风阀","止回阀 800×550","个",2]
[148,"风阀","止回阀 320×120","个",5]
[149,"风阀","止回阀 320*320","个",26]
[150,"风阀","止回阀 630X1200","个",2]
[151,"风阀","调节阀 250×120","个",50]
[152,"风阀","调节阀 250*160","个",25]
[153,"风阀","调节阀 200X120","个",46]
[154,"风阀","调节阀 630×250","个",1]
[155,"风阀","调节阀 200×160","个",3]
[156,"风阀","调节阀 800×400","个",1]
[157,"风阀","调节阀 400×200","个",9]
[158,"风阀","调节阀 320×160","个",22]
[159,"风阀","调节阀 400×250","个",8]
[160,"风阀","调节阀 320×200","个",19]
[161,"风阀","调节阀 160×120","个",4]
[162,"风阀","调节阀 160×160","个",1]
[163,"风阀","调节阀 500×250","个",3]
[164,"风阀","调节阀 120×120","个",1]
[165,"风阀","调节阀 500×320","个",9]
[166,"风阀","调节阀 320×120","个",28]
[167,"风阀","调节阀 320×250","个",7]
[168,"风阀","调节阀 400×320","个",5]
[169,"风阀","调节阀 630X320","个",1]
[170,"风阀","调节阀 500×400","个",1]
[171,"风阀","调节阀 500X200","个",4]
[172,"风阀","电动对开多叶调节阀 800×500","个",3]
[173,"风阀","电动对开多叶调节阀 630×630","个",2]
[174,"风阀","电动对开多叶调节阀 1000×400","个",1]
[175,"风阀","电动对开多叶调节阀 1250×400","个",1]
[176,"风阀","电动对开多叶调节阀 1000×500","个",3]
[177,"风阀","电动对开多叶调节阀 630X400","个",1]
[178,"风阀","电动对开多叶调节阀 630X250","个",2]
[179,"风口","BH/D 500×320","个",4]
[180,"风口","BH/D 500×250","个",1]
[181,"风阀","FD 500×250","个",7]
[182,"风阀","FD 400×320","个",6]
[183,"风阀","FD 500×320","个",3]
[184,"风阀","FD 800×400","个",1]
[185,"风阀","FD 400×250","个",4]
[186,"风阀","FD 320×200","个",4]
[187,"风阀","FD 250*160","个",6]
[188,"风阀","FD 320×250","个",4]
[189,"风阀","FD 500×400","个",1]
[190,"风阀","FD 1000×400","个",5]
[191,"风阀","FD 800×500","个",8]
[192,"风阀","FD 200×160","个",1]
[193,"风阀","FD 200X120","个",2]
[194,"风阀","FD 320×160","个",5]
[195,"风阀","FD 1000×500","个",4]
[196,"风阀","FD 1250×400","个",1]
[197,"风阀","FD 630X400","个",1]
[198,"风阀","FD 200*200","个",17]
[199,"风阀","FD 1000X630","个",2]
[200,"风阀","FD 500X400","个",2]
[201,"风阀","FD 630X1200","个",2]
[202,"风阀","FD 630X250","个",2]
[203,"风阀","FD 320×120","个",2]
[204,"风阀","FD 250×120","个",8]
[205,"风阀","FD 800X630","个",1]
[206,"风阀","FD 200*320","个",1]
[207,"风阀","FVD 160×120","个",1]
[208,"风阀","FVD 320×160","个",3]
[209,"风阀","FVD 320×200","个",2]
[210,"风阀","FVD 250*160","个",3]
[211,"风阀","FVD 250×120","个",1]
[212,"风阀","FVD 320×120","个",1]
[213,"风阀","FVD 400×200","个",1]
[214,"风阀","FVD 120×120","个",1]
[215,"风阀","FVD 200X120","个",2]
[216,"风阀","MEE 250*160","个",1]
[217,"风阀","MEE 320×200","个",1]
[218,"风阀","MEE 800×400","个",1]
[219,"风阀","MEE 500×400","个",1]
[220,"风阀","FDEH 1250×800","个",1]
[221,"风阀","FDEH 1600×630","个",3]
[222,"风阀","FDEH 800×500","个",1]
[223,"风阀","FDEH1250*900","个",1]
[224,"风阀","FDEH 800×400","个",1]
[225,"风阀","FDH 500×320","个",1]
[226,"风阀","FDH 1250×800","个",1]
[227,"风阀","FDH 1600×630","个",3]
[228,"风阀","FDH 500×250","个",2]
[229,"风阀","FDH 800×500","个",2]
[230,"风阀","FDH 800×550","个",2]
[231,"风阀","FDH 800×400","个",3]
[232,"风阀","BECH 500×320","个",9]
[233,"风阀","BECH 1000×500","个",18]
[234,"风阀","BECH 1000×550","个",9]
[235,"风阀","BECH 500×250","个",4]
[236,"风阀","BECH 1000×400","个",1]
[237,"风阀","BECH 630X320","个",10]
[238,"风阀","BECH 800×400","个",4]
[239,"风阀","BECH 500X400","个",7]
[240,"风阀","BECH 630X400","个",3]
[241,"风阀","BECH 400×320","个",2]
[242,"风阀","FDED 800×630","个",2]
[243,"风阀","FDED 800×550","个",2]
[244,"风阀","FDED 1600*550","个",1]
[245,"风阀","FDED 1600×630","个",1]
[246,"静压箱","静压箱 2850*500*400(h) ","个",1]
[247,"静压箱","送风静压箱1200*250*300","个",1]
[248,"静压箱","送风静压箱1400*250*300","个",1]
[249,"静压箱","送风静压箱1600*250*300","个",1]
[250,"静压箱","回风静压箱550*214*300","个",1]
[251,"静压箱","回风静压箱700*214*300","个",1]
[252,"静压箱","回风静压箱900*214*300","个",1]
[253,"静压箱","回风静压箱1000*214*300","个",1]
[254,"防火风口","GFE 300*400","个",1]
[255,"防火风口","GFE 800*400","个",1]
[256,"防火风口","GFE 500*1200","个",2]
[257,"防火风口","GFE 800*1200","个",2]
[258,"防火风口","GFE 1200*3000","个",5]
[259,"防火风口","GF 400*400","个",12]
[260,"防火风口","GF 200*800","个",1]
[261,"防火风口","GF 800*300","个",2]
[262,"防火风口","GF 800*600","个",1]
[263,"风口","百叶送风口-1000*137","个",13]
[264,"风口","百叶送风口-1200*103","个",14]
[265,"风口","百叶送风口-1400*103","个",12]
[266,"风口","百叶送风口-1400*137","个",21]
[267,"风口","百叶送风口-1400*171","个",2]
[268,"风口","百叶送风口-600*103","个",30]
[269,"风口","百叶送风口-700*103","个",12]
[270,"风口","百叶送风口-700*137","个",26]
[271,"风口","百叶送风口-800*69","个",14]
[272,"风口","可开百叶-带滤网回风口-1000*200","个",1]
[273,"风口","可开百叶-带滤网回风口-1200*200","个",1]
[274,"风口","可开百叶-带滤网回风口-800*200","个",1]
[275,"软接头","保温夹筋柔性软管","M2",1]
[276,"设备","减震器","个",1]
[null,"合计",{"$nulls":4},0]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}